{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":3,"macros":1,"external_links":0,"defined_names":30,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":15,"n_cols":9,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
["Oil and gas wells, Prof. Milan Stanko (NTNU)",null,null,null,null,"Inflow performance relationship (IPR)"]
[null,"pR [bara]","C [Sm3/bar2n]","n"]
["Layer 1",200,2010,0.52]
["Layer 2",250,1150,0.54]
[]
[null,"Cf [Sm3/d/bar]","s",null,null,"Tubing performance relationship (TPR)"]
["Tubing",2088.5376839201663,0.57687389850130322]
["Casing between 1-2",4000,1.8435523564968782E-2]
[]
[]
[]
[]
[null,"pwh","pwf1","qwell","q1","q2","pwf2 (from TPR)","pwf2 (from IPR)","error"]
[null,"[bara]","[bara]","[Sm3/d]","[Sm3/d]","[Sm3/d]","[bara]","[bara]","[bar]"]
[null,10,197.54168569001095]