{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["Column","y_vs_x","TEG_regeneration","Activity_coefficient"],"not_rendered":{"charts":3,"images":0,"macros":1,"external_links":0,"defined_names":33,"comments":0,"pivot_tables":0},"unopened":[{"sheet":"y_vs_x","index":1,"reason":"not_a_worksheet"}],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Column","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[]}
["Gas dehydration exercise, TPG4135, Prof. Milan Stanko"]
["gas rate",21,"1E06 Sm3/d"]
["Gas gg",0.65]
["p",52,"bara"]
["T",30,"C"]
["xo",0.02,"[-]"]
["gas sc molar density",{"$f":"101325/(8314*288*1)","v":4.2316925266618552E-2},"[Kmol/Sm3]"]
["MW water",18,"kg/Kmol"]
["TEG concentration",12,"l/kg H2O"]
["TEG density @ 25 C",1120,"kg/m3"]
["TEG MW",150.16999999999999,"kg/Kmol"]
["Desired dewpoint"]
["T",-10,"C"]
["p",52,"bara"]
[]
["rsw_inlet",null,"[kg/1e06 Sm3]"]
["rsw_outlet",null,"[kg/1e06 Sm3]"]
["m_water_to_remove",null,"[kg/d]"]
["n_water_to_remove",null,"[kmol/d]"]
[]
["G",null,"[kmol/d]",null,"[kmol/h]"]
["m_water_outlet_top",null,"[kg/d]"]
["n_water_outlet_top",null,"[kmol/d]"]
["y1",null,"[-]"]
["m_water_inlet_bottom",null,"[kg/d]"]
["n_water_inlet_bottom",null,"[kmol/d]"]
["yN+1",null,"[-]"]
["L",null,"[kmol/d]",null,"[kmol/h]"]
["xN",null,"[-]"]
[null,null,null,null,null,"k",5.0000000000000001E-4]
[null,"Operation line",null,null,null,"Equilibrium"]
[null,"x","y",null,"x","y"]

{"sheet":"TEG_regeneration","index":2,"n_rows":18,"n_cols":12,"rows_kept":18,"cut":false,"hidden":false,"merged":[]}
["T",{"$f":"206.6+273.15","v":479.75},"K"]
["p",124.325,"Kpa"]
[]
["Only TEG and Water"]
["Fv"]
[null,null,null,null,"pv","Z","K","RR_term","xi","yi","MW","Mass fraction"]
[null,"A","B","C","[Kpa]","[-]","[-]",null,"[-]","[-]"]
["H20",3.55959,643.74800000000005,-198.04300000000001]
["TEG",6.7568000000000001,3715.2220000000002,-1.2989999999999999]
[null,null,null,null,"sum=",null,"SUM="]
[]
[]
["n_TEG",null,"Kmol/d"]
["n_H2O",null,"Kmol/d"]
["n_total",null,"Kmol/d"]
["n_vapor",null,"Kmol/d"]
["n_vapor_TEG",null,"Kmol/d"]
["Makeup TEG",null,"kg/d"]

{"sheet":"Activity_coefficient","index":3,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":false,"merged":[]}
["weight % TEG","Activity coefficient"]
[92.460069318710794,0.74174745227872296]
[93.102519269566997,0.72276188505509198]
[93.611794526925607,0.70613367130515703]
[94.145362371320601,0.68831410687496697]
[94.691200662148802,0.66870027417101996]
[95.188702084734302,0.64907195696032205]
[95.625596192643897,0.63122342351663097]
[96.135368061662604,0.609800838032176]
[96.669618747090098,0.58538901246702102]
[97.155532564275006,0.56096270239511603]
[97.665925197868702,0.53354715224251203]
[98.1277326573896,0.50851430345041604]
[98.626165226837699,0.47989653923749398]
[99.015405307537094,0.45544126015208702]
[99.441208421705994,0.42800036211266801]
[99.794133774765896,0.40413351611401299]