{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Data","Pump_performance","pump_plot"],"not_rendered":{"charts":2,"images":0,"macros":1,"external_links":0,"defined_names":25,"comments":0,"pivot_tables":0},"unopened":[{"sheet":"pump_plot","index":2,"reason":"not_a_worksheet"}],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Data","index":0,"n_rows":14,"n_cols":13,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
["Problem 1 Undersaturated oil field, TPG4230 V2020, Resit exam, Prof. Milan Stanko "]
["Oil density, Rho",861,"kg/m3"]
["Oil viscosity(average), Vis",1.0300000000000001E-3,"Pa s",null,null,null,null,null,"Npumps",2,null,"eff",0.65]
["Pipeline data"]
["Horizontal pipe length",14000,"m","qwell","Pin","Priserbase","psep",null,"pwh","head","qpump","power"]
["Pipeline inner diameter, ID",{"$f":"8*0.0254","v":0.20319999999999999},"m","[Sm3/d]","[bara]","[bara]","[bara]",null,"[bara]","[m]","[Sm3/d]","[kW]"]
["Deviation angle  (from horizontal)",0,"deg",5000,{"$f":"pin(D7,B6,B2,B3,B5,B7,F7,B8)","v":49.528001699125838},{"$f":"pin(D7,B11,B2,B3,B10,90,G7,B13)","v":35.385371812823884},{"$f":"$B$14","v":20},null,20,{"$f":"(E7-I7)*100000/(B2*9.81)","v":349.59233211655408},{"$f":"D7/J3","v":2500},{"$f":"(K7/(3600*24))*J7*9.81*B2/(1000*M3)","v":131.44587650964138}]
["Pipeline roughness",1.5E-5,"m"]
["Riser data"]
["vertical pipe length",180,"m"]
["Flowline data diameter, ID",{"$f":"8*0.0254","v":0.20319999999999999},"m"]
["Deviation angle  (from horizontal)",90,"deg"]
["Riser roughness",1.5E-5,"m"]
["Separator Pressure",20,"bara"]

{"sheet":"Pump_performance","index":1,"n_rows":10,"n_cols":10,"rows_kept":10,"cut":false,"hidden":false,"merged":[]}
["RPM=",{"$f":"\"5500 rpm\"","v":"5500 rpm"},"RPM=",{"$f":"\"5000 rpm\"","v":"5000 rpm"},"RPM=",{"$f":"\"4500 rpm\"","v":"4500 rpm"},"RPM=",{"$f":"\"4000 rpm\"","v":"4000 rpm"},"RPM=",{"$f":"\"3500 rpm\"","v":"3500 rpm"}]
["rate [m3/d]","head [m]","rate [m3/d]","head [m]","rate [m3/d]","head [m]","rate [m3/d]","head [m]","rate [m3/d]","head [m]"]
[938.41042678251426,491.80859691808536,861.1295681063109,407.46147607461467,750.72834142601153,328.30494728304933,684.48760541783179,259.52960259529601,607.20674674163013,198.54014598540135]
[1633.9381548683818,484.0227088402267,1479.3764375159692,399.67558799675533,1413.1357015077897,324.41200324412,1236.4937388193164,255.636658556366,1092.9721441349336,194.64720194647199]
[2384.6664962944001,476.23682076236804,2185.9442882698672,393.18734793187338,2108.6634295936574,315.32846715328469,1876.8208535650349,249.14841849148402,1644.9782775364122,189.45660989456601]
[3157.4750830564772,446.3909164639087,2914.5923843598248,365.93673965936733,2704.8300536672618,291.97080291970804,2439.8671096345497,228.38605028386002,2196.9844109378969,173.88483373884802]
[3731.5614617940155,397.0802919708027,3400.3577817531295,328.30494728304933,3157.4750830564772,260.82725060827198,2870.4318936877048,199.83779399837735,2561.3084589828727,149.22952149229468]
[4261.4873498594407,338.68613138686061,3830.9225658062851,284.18491484184869,3510.7590084334233,224.49310624493066,3179.5553283925374,172.58718572587134,2859.3917710196743,124.57420924574201]
[4636.8515205724461,289.37550689375468,4217.3268591873211,241.36253041362536,3819.8824431382554,190.75425790754201,3632.2003577817522,129.76480129764801,3190.5954510605611,101.21654501216534]
[5023.2558139534822,243.95782643957801,4570.6107845642664,201.135442011354,4106.9256325070264,163.503649635036]