{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Data"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":25,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Data","index":0,"n_rows":8,"n_cols":4,"rows_kept":8,"cut":false,"hidden":false,"merged":[]}
["Problem 1 Undersaturated oil field, TPG4135 V2020, Resit exam, Prof. Milan Stanko "]
["Pipe diameter",0.1,"m","Input is red"]
["fluid velocity",2,"m/s","Output is blue"]
["pipe roughness",1.5E-5,"m"]
["Oil density, Rho",861,"kg/m3"]
["Oil viscosity(average), Vis",1.0300000000000001E-3,"Pa s"]
[]
["friction factor",{"$f":"ffactor(B5,B6,B2,B4,B3)","v":1.6984893850168898E-2},"[-]"]