{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Multiphase"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Multiphase","index":0,"n_rows":19,"n_cols":6,"rows_kept":19,"cut":false,"hidden":false,"merged":[]}
["Multiphase calculator, TPG4230, Prof. Milan Stanko, "]
["FLUID PROPERTIES"]
[]
["μo","[Pa s]",2.09460052895507E-4]
["μg","[Pa s]",1.7871571391003901E-5]
["σog","[N/m]",8.5856773799709105E-3]
["ρo","[kg/m^3]",569.37143860094]
["ρg","[kg/m^3]",115.772189269721,null,"dp/dx","Flow pattern"]
[null,null,null,null,"[Pa/m]","[-]"]
["OPERATING CONDITIONS",null,null,null,{"$f":"multiphasedpdx($C$12,$C$13,$C$8,$C$7,$C$5,$C$4,$C$18,$C$17,$C$6,$C$19)","v":5659.5992299639756},"Bubble"]
[]
["Usl","[m/s]",1.851134551725852]
["Usg","[m/s]",2.0072829707194387E-2]
[]
["PIPING CHARACTERISTICS"]
[]
["Angle (from hor.)","[rad]",{"$f":"90*PI()/180","v":1.5707963267948966}]
["Diameter","[m]",0.12]
["Roughness","[m]",1.5E-5]