{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Data"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":37,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Data","index":0,"n_rows":16,"n_cols":7,"rows_kept":16,"cut":false,"hidden":false,"merged":[]}
["PRODUCTION OTIMIZATION"]
["5 Well Optimization Problem"]
["Well ","qmaxo","WC","GOR","qo","qg","qw"]
[null,"Sm3/D","fraction","Sm3/m3","Sm3/D","Sm3/D","Sm3/D"]
[1,635.6,0.2,142]
[2,794.5,0.43,213.6]
[3,476.7,0.31,267]
[4,635.6,0.47,356]
[5,317.8,0.1,249.2]
[null,null,null,"qototal [Sm3/d]"]
[]
["Constraints Separator"]
["qo","No Limit","Sm3/d","Maximize oil production"]
["qw ",795,"Sm3/d"]
["qg ",283000,"Sm3/d"]
["qo min ",50,"Sm3/d"]