{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":9,"n_cols":10,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
["Prof. Milan Stanko (NTNU)"]
["Inflow",null,null,null,null,"qg","[Sm3/d]",2500000,null,"Red is input"]
["CR","[Sm3/d/bar2n]",104,null,null,"pR","[bara]",304,null,"Blue is calculated"]
["n","[-]",0.9,null,null,"pwf","[bara]"]
["Tubing",null,null,null,null,"pwh","[bara]"]
["CT","[Sm3/d/bar]",44100,null,null,"pin","[bara]"]
["S","[-]",0.31,null,null,"Dpchoke","[bar]"]
["Flowline",null,null,null,null,"psep","[bara]",40]
["Cfl","[Sm3/d/bar]",40000]