{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["CALC"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":31,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"CALC","index":0,"n_rows":9,"n_cols":10,"rows_kept":9,"cut":false,"hidden":false,"merged":[[0,1,0,5]]}
[null,"Gas lift performance curve coefficients"]
[null,"a","b","c","d","e","qg_inj","qo","Reservoir GOR","qg_total"]
[null,"[(1/Sm3/d)3]","[(1/Sm3/d)2]","[1/Sm3/d]",null,"[Sm3/d]","[1E03 Sm3/d]","[Sm3/d]","[Sm3/Sm3]","[1E03 Sm3/d]"]
["Well 1",-3.9000000000000002E-7,2.1000000000000001E-4,-4.2999999999999997E-2,3.7,12,null,null,100]
["Well 2",-1.3E-7,1E-4,-2.8000000000000001E-2,3.1,-17,null,null,200]
[null,null,null,null,null,"TOTAL="]
[]
["qg_inj_max","[1E03 Sm3/d]",130]
["qg_max_sep","[1E03 Sm3/d]",150]