{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Task_1","Task_2","Task_3"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":99,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Task_1","index":0,"n_rows":9,"n_cols":10,"rows_kept":9,"cut":false,"hidden":false,"merged":[[0,1,0,5]]}
[null,"Gas lift performance curve coefficients"]
[null,"a","b","c","d","e","qg_inj","qo","Reservoir GOR","qg_total"]
[null,"[(1/Sm3/d)3]","[(1/Sm3/d)2]","[1/Sm3/d]",null,"[Sm3/d]","[1E03 Sm3/d]","[Sm3/d]","[Sm3/Sm3]","[1E03 Sm3/d]"]
["Well 1",-3.9000000000000002E-7,2.1000000000000001E-4,-4.2999999999999997E-2,3.7,12,83.747589419330481,{"$f":"qo_r(G4,B4,C4,D4,E4,F4)","v":124.44327837331323},100,{"$f":"(I4*H4/1000)+G4","v":96.19191725666181}]
["Well 2",-1.3E-7,1E-4,-2.8000000000000001E-2,3.1,-17,98.311580639358411,{"$f":"qo_r(G5,B5,C5,D5,E5,F5)","v":100.01700188573082},200,{"$f":"(I5*H5/1000)+G5","v":118.31498101650457}]
[null,null,null,null,null,"TOTAL=",{"$f":"SUM(G4:G5)","v":182.05917005868889},{"$f":"SUM(H4:H5)","v":224.46028025904405},null,{"$f":"SUM(J4:J5)","v":214.50689827316637}]
[]
["qg_inj_max","[1E03 Sm3/d]",133]
["qg_max_sep","[1E03 Sm3/d]",150]

{"sheet":"Task_2","index":1,"n_rows":9,"n_cols":10,"rows_kept":9,"cut":false,"hidden":false,"merged":[[0,1,0,5]]}
[null,"Gas lift performance curve coefficients"]
[null,"a","b","c","d","e","qg_inj","qo","Reservoir GOR","qg_total"]
[null,"[(1/Sm3/d)3]","[(1/Sm3/d)2]","[1/Sm3/d]",null,"[Sm3/d]","[1E03 Sm3/d]","[Sm3/d]","[Sm3/Sm3]","[1E03 Sm3/d]"]
["Well 1",-3.9000000000000002E-7,2.1000000000000001E-4,-4.2999999999999997E-2,3.7,12,59.98774808940486,{"$f":"qo_r(G4,B4,C4,D4,E4,F4)","v":119.49982681472991},100,{"$f":"(I4*H4/1000)+G4","v":71.937730770877849}]
["Well 2",-1.3E-7,1E-4,-2.8000000000000001E-2,3.1,-17,70.012251912999162,{"$f":"qo_r(G5,B5,C5,D5,E5,F5)","v":93.984476867880261},200,{"$f":"(I5*H5/1000)+G5","v":88.809147286575211}]
[null,null,null,null,null,"TOTAL=",{"$f":"SUM(G4:G5)","v":130.00000000240402},{"$f":"SUM(H4:H5)","v":213.48430368261018},null,{"$f":"SUM(J4:J5)","v":160.74687805745305}]
[]
["qg_inj_max","[1E03 Sm3/d]",130]
["qg_max_sep","[1E03 Sm3/d]",150]

{"sheet":"Task_3","index":2,"n_rows":9,"n_cols":10,"rows_kept":9,"cut":false,"hidden":false,"merged":[[0,1,0,5]]}
[null,"Gas lift performance curve coefficients"]
[null,"a","b","c","d","e","qg_inj","qo","Reservoir GOR","qg_total"]
[null,"[(1/Sm3/d)3]","[(1/Sm3/d)2]","[1/Sm3/d]",null,"[Sm3/d]","[1E03 Sm3/d]","[Sm3/d]","[Sm3/Sm3]","[1E03 Sm3/d]"]
["Well 1",-3.9000000000000002E-7,2.1000000000000001E-4,-4.2999999999999997E-2,3.7,12,56.285351018843862,{"$f":"qo_r(G4,B4,C4,D4,E4,F4)","v":117.56181881148291},100,{"$f":"(I4*H4/1000)+G4","v":68.041532899992148}]
["Well 2",-1.3E-7,1E-4,-2.8000000000000001E-2,3.1,-17,63.830152931562658,{"$f":"qo_r(G5,B5,C5,D5,E5,F5)","v":90.641666150542591},200,{"$f":"(I5*H5/1000)+G5","v":81.958486161671175}]
[null,null,null,null,null,"TOTAL=",{"$f":"SUM(G4:G5)","v":120.11550395040652},{"$f":"SUM(H4:H5)","v":208.2034849620255},null,{"$f":"SUM(J4:J5)","v":150.00001906166332}]
[]
["qg_inj_max","[1E03 Sm3/d]",133]
["qg_max_sep","[1E03 Sm3/d]",150]