{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Data"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":39,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Data","index":0,"n_rows":14,"n_cols":9,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
["Problem 2, Resit Exam TPG4230, V2020, Prof. Milan Stanko"]
[]
["Well ","qlmin","qlmax","Coning coefficient C","ql_critical","ql","WC","qo","qw"]
[null,"[Sm3/d]","[Sm3/d]","[1/Sm3/d]","[Sm3/d]","[Sm3/d]","[-]","[Sm3/d]","[Sm3/d]"]
[1,211.86666666666667,635.6,1.012,91.3,211.86666666666667,{"$f":"Wc(E5,D5,F5)","v":0.49866546782191684},{"$f":"F5-I5","v":106.21607621746323},{"$f":"F5*G5","v":105.65059044920345}]
[2,264.83333333333331,794.5,1.012,61.03,512.27834633903569,{"$f":"Wc(E6,D6,F6)","v":0.71187020908102183},{"$f":"F6-I6","v":147.60265282298622},{"$f":"F6*G6","v":364.67569351604948}]
[3,158.9,476.7,1.012,35.06,476.7,{"$f":"Wc(E7,D7,F7)","v":0.70946409976379698},138.49846364259798,338.20153635740201]
[4,211.86666666666667,635.6,1.012,55.3,571.42167876756832,{"$f":"Wc(E8,D8,F8)","v":0.72609721659543736},156.51398831214482,414.90769045542351]
[5,105.93333333333334,317.8,1.012,76.42,290.76338116685491,{"$f":"Wc(E9,D9,F9)","v":0.60724574450134405},114.19855529646003,176.56482587039488]
[null,null,null,null,null,null,"qtotal [Sm3/d]",{"$f":"SUM(H5:H9)","v":663.02973629165217},{"$f":"SUM(I5:I9)","v":1400.0003366484734}]
[]
["Constraints Separator"]
["qo","No Limit","Sm3/d","Maximize oil production"]
["qw ",1400,"Sm3/d"]