{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Data"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":28,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Data","index":0,"n_rows":17,"n_cols":10,"rows_kept":17,"cut":false,"hidden":false,"merged":[]}
["Problem 2, Re-sit examination, Prof. Milan Stanko (NTNU)"]
[]
["GOR","[Sm3/Sm3]",150]
["pin,pipeline","[bara]",120]
["uptime","[d/year]",365]
["deno,sc","[kg/m3]",800]
["deng,sc","[kg/m3]",0.8]
["hadia,MPP","[-]",0.6]
[]
["time (end of year)","qo target","Np","pinlet,subseastation","qo avail","pin,pipe","Dpchoke\nDpMPP","mass flow","Dhs","Power, MPP"]
["[years]","[sm3/d]","[Sm3]","[bara]","[sm3/d]","[bara]","[bar]","[kg/s]","[kJ/kg]","[kW]"]
[0,2531]
[1,2531]
[2,2531]
[3,2487]
[4,2436]
[5,2467]