{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Data_res_well_network","Field Layout","Equations list"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":1,"defined_names":48,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Data_res_well_network","index":0,"n_rows":23,"n_cols":16,"rows_kept":23,"cut":false,"hidden":false,"merged":[]}
["Snohvit Gas Field, Prof. Michael Golan, Prof. Milan Stanko"]
[" G (IGIP), Initial gas in place",{"$f":"270000000000","v":270000000000},"[Sm3]"]
["Production days per year (uptime)",360,"[day]",null,null,null,null,"i.e same PR CR, n, Ct, S"]
["TR , reservoir temperature",92,"[°C]",null,null,null,null,"2. System is symmetric"]
["pRi, initial reservoir pressure",276,"[bara]",null,null,null,null,"3. Field Rate = 20 MMSCM"]
["CR, inflow backpressure coefficient",1000,"[Sm3/bar^2n]",null,null,null,null,"qwell = qg/no.of.wells"]
["n, inflow backpressure exponent",1,"[-]",null,null,null,null,"PR= ZR* P/Zi * (1-Gp/G)"]
["Ct, Tubing flow coefficient (2100 MDx0.15 ID  m)",40288.195917865203,"[Sm3/bar]",null,null,null,null,"Pwf = sqrt(Pr^2-qg/C) as n=1"]
["S, Tubing elevation coefficient",0.155,"[-]",null,null,null,null,"Pwh = sqrt((pwf^2/e^s)-((qg/Ct)^2))"]
["CFL , flowline coefficient from template-PLEM (5000x0.355  ID m)",283126.86618411407,"[Sm3/bar]",null,null,null,null,"Psep"]
["CPL Pipeline coefficient from PLEM-Shore (158600x0.68  ID m)",275064.39272584103,"[Sm3/bar]",null,null,null,null,"Pplem"]
["Separator  (slug catcher) pressure",30,"[bara]",null,null,null,null,"Ptempl"]
["Gas molecular weight (Methane)",16,"[kg/kmole]"]
["Gas specific gravity",{"$f":"$B$13/28.93","v":0.55305910819218806},"[-]"]
["Gas density at Sc",{"$f":"101325/((8314/(0.55*28.97))*(273.15+15.56))","v":0.67259858638728143},"[kg/m^3]"]
["Number of templates",3]
["Number of wells per template",3]
["qfield",20000000,"[Sm^3/d]"]
[]
[null,"time","qfield","DGp","Gp","Rf","Z","pR","qwell","pwf","pwh","ptemp ","pplem","psep","qtemp","Dpchoke"]
[null,"[years]","[Sm^3/d]","[Sm^3]","[Sm^3]","[-]","[-]","[bara]","[Sm^3/d]","[bara]","[bara]","[bara]","[bara]","[bara]","[Sm^3/d]","[bar]"]
[null,0]
[null,1]

{"sheet":"Field Layout","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Equations list","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}