{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Production_schedule","Network_solving"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":28,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Production_schedule","index":0,"n_rows":22,"n_cols":7,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
[]
[" G (IGIP), Initial gas in place",{"$f":"200000000","v":200000000},"[Sm3]"]
["Production days per year (uptime)",360,"[day]"]
["pRi, initial reservoir pressure",150,"[bara]"]
["qfield desired",100000,"[Sm^3/d]"]
["Field gas rate for abandonment (1/3 of plateau rate)",{"$f":"B5/3","v":33333.333333333336},"[Sm^3/d]"]
[]
[null,"time","qfield","DGp","Gp","Rf","pR"]
[null,"[years]","[Sm^3/d]","[Sm^3]","[Sm^3]","[-]","[bara]"]
[null,0]
[null,1]
[null,2]
[null,3]
[null,4]
[null,5]
[null,6]
[null,7]
[null,8]
[null,9]
[null,10]
[null,11]
[null,12]

{"sheet":"Network_solving","index":1,"n_rows":10,"n_cols":13,"rows_kept":10,"cut":false,"hidden":false,"merged":[[3,2,3,3],[3,4,3,5]]}
[]
["Network of two gas wells"]
[]
[null,null,"IPR",null,"Tubing",null,"Flowline"]
["Component Name","pR","C","n","S","Ct","Cfl","psep","pwf","qwell","pwh","pjunc","error"]
[null,"[bara]","[Sm^3/bar^2n]",null,null,"[Sm^3/bar^2]","[Sm^3/bar^2]","[bara]","[bara]","[Sm^3/d]","[bara]","[bara]","(bara^2)"]
["W_1",44.479888277826284,52,0.8,0.13,7680,8673]
["W_2",44.479888277826284,40,0.75,0.11,8600,7563]
["Pipeline",null,null,null,null,null,14080,28.6]
[null,null,null,null,null,null,null,null,null,null,"Average="]