{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Data"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Data","index":0,"n_rows":30,"n_cols":10,"rows_kept":30,"cut":false,"hidden":false,"merged":[]}
["Problem 1, Exam H2021, TPG4245, Prof. Milan Stanko (NTNU)"]
[]
["Data - fluid and reservoir",null,null,null,"Data - Tubing"]
["pR","[bara]",350,null,"Ct, tubing","[Sm3/d/bar]",42500,{"$f":"G4*((0.1/0.154)^2.61)","v":13770.821492018104}]
["TR","[C]",100,null,"s, elevation coeff","[-]",0.155]
["TR","[K]",{"$f":"C5+273.15","v":373.15}]
["zR","[-]",1.0104344304518729,null,"Data - Flowline"]
["dengR","[kg/m3]",226.41088715394076,null,"Cfl, flowline","[Sm3/d/bar]",40000]
["ViscosityR","[cp]",2.6617212334593351E-2,null,"psep","[bara]",40]
["re","[m]",500]
["rw","[m]",0.1,null,"SOLUTION"]
["s, skin","[-]",5,null,"m(pR)","[bara2/cp]",{"$f":"tabinterpol($C$4,2,A19:B26)","v":6394301.8075255128}]
["k","[md]",10,null,"Q1"]
["h","[m]",100,null,"pwf","m(pwf)","qg","pwh","pin","DP choke"]
["SGg","[-]",0.7,null,"[bara]","[bara2/cp]","[Sm3/d]","[bara]","[bara]","[bara]"]
[null,null,null,null,289.43738471306477,{"$f":"tabinterpol(E16,2,A19:B26)","v":4833332.5613338454},{"$f":"ipr_gas_qg($C$13,$C$14,$C$6,$C$10,$C$11,$C$12,G12,F16)","v":2500000},{"$f":"Tubingp2($G$4,$G$5,E16,G16)","v":261.31421159792171},{"$f":"linep1(G8,G9,G16)","v":74.204110398279155},{"$f":"H16-I16","v":187.11010119964254}]
["p","m(p)"]
["bara","[bara2/cp]",null,null,"From chart, Tin = 32 C"]
[1.01325,0]
[50,186685.26994467882]
[100,732314.48107347253,null,null,"Q2"]
[150,1579684.201363584]
[200,2642729.9716099892,null,null,"pwf","m(pwf)","qg","pwh","pin","DP choke"]
[250,3836936.9466185668,null,null,"[bara]","[bara2/cp]","[Sm3/d]","[bara]","[bara]","[bara]"]
[300,5100199.7389725354,null,null,211.31254285268039,{"$f":"tabinterpol(E25,2,A19:B26)","v":2912920.3232050762},{"$f":"ipr_gas_qg($C$13,$C$14,$C$6,$C$10,$C$11,$C$12,G12,F25)","v":5575672.7635955084},{"$f":"Tubingp2($G$4,$G$5,E25,G25)","v":145.01751394074532},{"$f":"linep1(G8,G9,G25)","v":145.01751352573933},{"$f":"H25-I25","v":4.1500598513266596E-7}]
[{"$f":"C4","v":350},6394301.8075255128]
[null,null,null,null,"Q3"]
[null,null,null,null,"pwf","m(pwf)","qg","pwh","pin","DP choke"]
[null,null,null,null,"[bara]","[bara2/cp]","[Sm3/d]","[bara]","[bara]","[bara]"]
[null,null,null,null,271.42449379831334,{"$f":"tabinterpol(E30,2,A19:B26)","v":4378232.263827119},{"$f":"ipr_gas_qg($C$13,$C$14,$C$6,$C$10,$C$11,$C$12,G12,F30)","v":3228874.541598185},{"$f":"Tubingp2($H$4,$G$5,E30,G30)","v":90.088724282515244},{"$f":"linep1(G8,G9,G30)","v":90.088951894020042},{"$f":"H30-I30","v":-2.2761150479766457E-4}]