{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Data"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":7,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Data","index":0,"n_rows":6,"n_cols":6,"rows_kept":6,"cut":false,"hidden":false,"merged":[]}
["Problem 5, Exam TPG4245, Prof. Milan Stanko"]
["pR, Res pressure",120,"bara"]
["Ct, tubing flow coefficient",7680,"Sm3/d/bar",null,"Test point"]
["s, tubing elevation coefficient",0.13,null,null,"qg","pwf"]
["pwh",13,"bara",null,"[Sm3/d]","[bara]"]
[null,null,null,null,68900,80]