{"text_format":"1","workbook":"xlsx","n_sheets":7,"sheets":["Data_Standalone","Plot_Standalone","Plot_Standalone (2)","Data_IPR_only","Data_IPR_changing_pwf","Data_Network","Plot_Std_vs_IPR_vs_net"],"not_rendered":{"charts":6,"images":0,"macros":1,"external_links":0,"defined_names":132,"comments":0,"pivot_tables":0},"unopened":[{"sheet":"Plot_Standalone","index":1,"reason":"not_a_worksheet"},{"sheet":"Plot_Standalone (2)","index":2,"reason":"not_a_worksheet"},{"sheet":"Plot_Std_vs_IPR_vs_net","index":6,"reason":"not_a_worksheet"}],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Data_Standalone","index":0,"n_rows":44,"n_cols":29,"rows_kept":44,"cut":false,"hidden":false,"merged":[]}
["CONFIGURATION: Standalone wells",null,null,null,null,"RESULTS"]
["Reservoir",null,null,null,null,"base case",null,"psep + 66%",null,"psep - 66%",null,"dtub + 50%",null,"dtub - 50%",null,"k h + 50%",null,"k h - 50%",null,"pi + 36%",null,"pi - 36%",null,"TR - 22%",null,"TR + 22%",null,"Sg + 50%"]
["G",270000000000,"[Sm3]",null,null,"RF","qpp_n","RF","qpp_n","RF","qpp_n","RF","qpp_n","RF","qpp_n","RF","qpp_n","RF","qpp_n","RF","qpp_n","RF","qpp_n","RF","qpp_n","RF","qpp_n","RF","qpp_n"]
["n",1,"[-]",null,null,"[-]","[-]","[-]","[-]","[-]","[-]","[-]","[-]","[-]","[-]","[-]","[-]","[-]","[-]","[-]","[-]","[-]","[-]","[-]","[-]","[-]","[-]","[-]","[-]"]
["pi",{"$f":"(1)*276","v":276},"[bara]",null,null,0,1,0,1,0,1,0,1,0,1,0,1,0,1,0,1,0,1,0,1,0,1,0,1]
["TR",90,"[C]",null,null,7.8171458235153368E-2,0.90155024703746534,7.8171458235153368E-2,0.89709993320722137,7.8171458235153368E-2,0.90289371343545244,7.8171458235153368E-2,0.90005702578241631,7.8171458235153368E-2,0.90814737591770145,7.8171458235153368E-2,0.9033393299296546,7.8171458235153368E-2,0.89500122277064043,6.629588792127572E-2,0.90639860644380332,8.9602202110266038E-2,0.89159258077823111,7.6605488274344213E-2,0.90237166542104219,7.9208075365014841E-2,0.90003755974883282,6.7574460826642868E-2,0.90427021577906908]
["Sg",0.5,"[-]",null,null,0.1608627327821176,0.80202566034403733,0.1608627327821176,0.79333675041645879,0.1608627327821176,0.80504367969170598,0.1608627327821176,0.79933724690539998,0.1608627327821176,0.81452767120402403,0.1608627327821176,0.80586512574848113,0.1608627327821176,0.78880884588530931,0.13860038009704767,0.81146576277735494,0.18070331829280428,0.78256534963224611,0.15845475012618937,0.80376611239840468,0.1623896986404737,0.79917141874671282,0.14270771463510856,0.80759167829033651]
["Well",null,null,null,null,0.24781137811331755,0.70147172492776355,0.24781137811331755,0.68845759772997761,0.24781137811331755,0.70653751983141944,0.24781137811331755,0.69786081415065715,0.24781137811331755,0.7192851765860494,0.24781137811331755,0.70760014059334231,0.24781137811331755,0.68156615901450812,0.2173697346715503,0.71521762127631561,0.27289240791957126,0.67292664156148418,0.24531064737640729,0.70421151863632425,0.2492946862690224,0.69747866528499558,0.22586967769081756,0.70994484376754285]
["skin",3,"[-]",null,null,0.33850852012316635,0.59992355839580702,0.33850852012316635,0.58208252537206484,0.33850852012316635,0.60748397279288802,0.33850852012316635,0.59560691337034299,0.33850852012316635,0.62258823652448592,0.33850852012316635,0.60853129090243319,0.33850852012316635,0.5734785177972358,0.30280876905933141,0.61769983520936045,0.36573356759968467,0.56254578920974529,0.33659088076734678,0.60365275324927758,0.33949163011239269,0.59500616248742044,0.31689685410019564,0.61116971136948628]
["external radius, re",453.85,"[m]",null,null,0.43219357131538294,0.49743908006202975,0.43219357131538294,0.47365671928530129,0.43219357131538294,0.5080780569544705,0.43219357131538294,0.49255351609058479,0.43219357131538294,0.52458070564932135,0.43219357131538294,0.50862820178332213,0.43219357131538294,0.4649152888268307,0.39468507347013415,0.51895023821891784,0.45878482278169286,0.45132149186632586,0.43134562403677679,0.50207644851697575,0.43236731451082955,0.49180370630357118,0.41464538885544167,0.51102028586024051]
["wellbore radius",0.11,"[m]",null,null,0.52789586008125666,0.39397027255353845,0.52789586008125666,0.36207504906252819,0.52789586008125666,0.4085421567878032,0.52789586008125666,0.3886452158102362,0.52789586008125666,0.42527735255956384,0.52789586008125666,0.40768436646355416,0.52789586008125666,0.35648161615896923,0.49215517888866878,0.41900691283355762,0.55161669561411286,0.33887824032534192,0.52831680347038135,0.39935662623821239,0.52715460950536319,0.38788216914366114,0.51687406598790775,0.40908716650361088]
["kh",{"$f":"1*2030","v":2030},"[md m]",null,null,0.62452185176761266,0.28940017765606191,0.62452185176761266,0.24501240090073231,0.62452185176761266,0.30933522352463771,0.62452185176761266,0.28380427837249789,0.62452185176761266,0.32436625002385455,0.62452185176761266,0.30527891380220246,0.62452185176761266,0.24930734083249212,0.5937074429073057,0.31787085490484379,0.64382830889945475,0.22450067645508612,0.62607952337395445,0.29521047270536011,0.62298812862104336,0.28321301500344587,0.62058586785883563,0.30473420215245872]
["Field",null,null,null,null,0.72096740372694046,0.18318637780667515,0.72096740372694046,0.11520678300241116,0.72096740372694046,0.2112605591816076,0.72096740372694046,0.17771395741115317,0.72096740372694046,0.22032186725268391,0.72096740372694046,0.20008019864189214,0.72096740372694046,0.14554184590533273,0.69731761560710592,0.21536807228945895,0.73505948432415558,0.10624591510648561,0.72322442857705871,0.18879720731873564,0.7189771247492085,0.17749585573594573,0.72273794580091022,0.19620448245091995]
["psep",{"$f":"(1)*30","v":30},"bara",null,null,0.87362122834455058,0,0.78645506097668116,0,0.95848040963376768,0,0.87378168775119325,0,0.87362122834455058,0,0.87362122834455058,0,0.87362122834455058,0,0.90017994530035317,0,0.81000889464996662,0,0.8749350756093387,0,0.87257994716033749,0,0.86749849552794411,0]
["Nw",5,"[-]"]
["Tubing",null,null,null,null,"for RF=0.625"]
["Tubing TVD",3000,"[m]",null,null,"max dev ","[%]",{"$f":"ABS(G12-O12)*100/G12","v":12.082256704537386}]
["Internal Diameter",{"$f":"0.15*1","v":0.15},"[m]",null,null,"min dev","[%]",{"$f":"ABS(G12-K12)*100/G12","v":6.8884013928518186},null,null,null,null,"Instructions to solve"]
["A",{"$f":"0.25*PI()*B18^2","v":1.7671458676442587E-2},"[m2]",null,null,null,null,null,null,null,null,null,{"$f":"\"1. Provide a suitable seed in column D (e.g. 5 bara less than pR)\"","v":"1. Provide a suitable seed in column D (e.g. 5 bara less than pR)"}]
["L",3000,"[m]",null,null,null,null,null,null,null,null,null,{"$f":"\"2. click solve all to find maximum rates\"","v":"2. click solve all to find maximum rates"}]
["Twh",70,"[C]",null,null,null,null,null,null,null,null,null,{"$f":"\"3. copy column L to G (values only). If psep or pwh change significantly, repeat from step 2.\"","v":"3. copy column L to G (values only). If psep or pwh change significantly, repeat from step 2."}]
["Friction factor",{"$f":"ff($B$18)","v":1.1777314787101792E-2},"[-]"]
["Sound speed at wh",{"$f":"SQRT(k_const(B7)*8314*(B21+273.15)/(B7*28.93))","v":509.3698309516567},"[m/s]"]
["Flowline",null,null,null,null,null,null,null,"From:",{"$f":"ROW(A35)","v":35}]
["L",10000,"[m]",null,null,null,null,null,"To:",{"$f":"ROW(A44)","v":44}]
["Tsep",60,"[C]"]
["Internal Diameter",{"$f":"6*25.4/1000","v":0.15239999999999998},"[m]"]
["A",{"$f":"0.25*PI()*B27^2","v":1.8241469247509915E-2},"[m2]"]
["Friction factor",{"$f":"ff($B$27)","v":1.1735513370070387E-2},"[-]"]
["Zsep",{"$f":"ZfacStanding($B$14,$B$26,$B$7,2)","v":0.97138593747056057},"[-]"]
["Sound speed at sep",{"$f":"SQRT(k_const(B7)*8314*(B26+273.15)/(B7*28.93))","v":501.89298563752271},"[m/s]"]
[null,null,null,"Guess (solver)",null,null,"Guess (manual)",null,null,null,null,"2. Paste to G"]
["pR","RF","ZR","pwf","qwell","Zwf","pwh","Zwh","Zav_Tub","S","CT","pwh","Mch at wh","Cflow","psep","Mch at sep","qfield","qpp_n"]
["[bara]","[-]","[-]","[bara]","[Sm3/d]","[-]","[bara]","[-]","[-]","[-]","Sm3/bar","[bara]","[-]","Sm3/bar ","[bara]","[-]","[Sm3/d]","[-]"]
[{"$f":"$B$5","v":276},{"$f":"MBgastank_RF($A$35,$C$35,C35,A35)","v":0},{"$f":"ZfacStanding(A35,$B$6,$B$7,2)","v":0.97949102344801509},241.34478249725709,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A35,$B$6,$B$7),m_function(D35,$B$6,$B$7))","v":3949405.2594603114},{"$f":"ZfacStanding(D35,$B$6,$B$7,2)","v":0.96146536226100399},182.54257635955025,{"$f":"ZfacStanding(G35,$B$21,$B$7,2)","v":0.91977059455543564},{"$f":"(H35+F35)*0.5","v":0.94061797840821981},{"$f":"s($B$7,(($B$21+$B$6)*0.5)+273.15,I35,$B$17)","v":0.30869678993799765},{"$f":"Cflowconst($B$18,$B$7,$B$22,I35,(($B$21+$B$6)*0.5)+273.15,$B$20,J35)","v":40631.980815398856},{"$f":"Tubingp2(K35,J35,D35,E35)","v":182.56311332807365},{"$f":"(Bg(G35,$B$21,H35,2)*E35/($B$19*24*3600))/$B$23","v":3.0815305195833878E-2},{"$f":"Cflowconst($B$27,$B$7,$B$29,(H35+$B$30)*0.5,(($B$26+$B$21)*0.5)+273.15,$B$25,0)","v":21931.229542617468},{"$f":"linep2(N35,L35,E35)","v":30.000006985305699},{"$f":"(Bg(O35,$B$26,$B$30,2)*E35/($B$28*24*3600))/$B$31","v":0.18902187885228275},{"$f":"E35*$B$15","v":19747026.297301557},{"$f":"Q35/$Q$35","v":1}]
[{"$f":"A35+(-$A$35/11)","v":250.90909090909091},{"$f":"MBgastank_RF($A$35,$C$35,C36,A36)","v":7.8171458235153368E-2},{"$f":"ZfacStanding(A36,$B$6,$B$7,2)","v":0.96595662274458938},218.00832559354549,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A36,$B$6,$B$7),m_function(D36,$B$6,$B$7))","v":3559215.2705594557},{"$f":"ZfacStanding(D36,$B$6,$B$7,2)","v":0.9522153918574674},164.98902938173632,0.91847515919381495,{"$f":"(H36+F36)*0.5","v":0.93534527552564117},0.31043696706481766,40763.16142027406,{"$f":"Tubingp2(K36,J36,D36,E36)","v":164.98467763284043},{"$f":"(Bg(G36,$B$21,H36,2)*E36/($B$19*24*3600))/$B$23","v":3.0682167144444005E-2},21938.744810111388,{"$f":"linep2(N36,L36,E36)","v":29.999999364029822},{"$f":"(Bg(O36,$B$26,$B$30,2)*E36/($B$28*24*3600))/$B$31","v":0.17034709896671937},{"$f":"E36*$B$15","v":17796076.352797277},{"$f":"Q36/$Q$35","v":0.90120284871596701}]
[{"$f":"A36+(-$A$35/11)","v":225.81818181818181},0.1608627327821176,0.9550305745739005,194.59391247449986,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A37,$B$6,$B$7),m_function(D37,$B$6,$B$7))","v":3165345.611478522},0.94557504055750763,147.41600965545342,0.91928283805868061,0.93242893930809412,0.31140791351676755,40836.257178408632,147.39716463662774,3.0566454398143889E-2,21934.058279730685,29.999997333404163,0.1514961691415945,15826728.05739261,0.80147399507719008]
[200.72727272727272,{"$f":"MBgastank_RF($A$35,$C$35,C38,A38)","v":0.24781137811331766},0.94704584360159316,171.10930126500918,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A38,$B$6,$B$7),m_function(D38,$B$6,$B$7))","v":2767904.0845761918},0.94178382036815711,129.82807449208312,0.92220861458680892,0.93199621747748296,0.3115524988700949,40847.136052767986,129.80400221190396,3.0446054701493162E-2,21917.106667593744,29.999986793163018,0.13247432165732442,13839520.422880959,0.70084073492990373]
[175.63636363636363,0.33850852012316635,0.94228344344355919,147.57692165789473,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A39,$B$6,$B$7),m_function(D39,$B$6,$B$7))","v":2366933.2363842418},0.941003507432568,112.2436087977057,0.92720978593504166,0.93410664668380483,0.31084860762250316,40794.159451757594,112.22153682797133,3.0277626077590779E-2,21888.221243841886,29.999946577479779,0.11328365638739588,11834666.18192121,0.59931384117002084]
[150.54545454545453,0.43219357131538294,0.94093304334248529,124.06153145347935,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A40,$B$6,$B$7),m_function(D40,$B$6,$B$7))","v":1962547.5911673631},0.94328074797230066,94.719393782025975,0.93417159102405367,0.93872616949817722,0.30931890462562639,40678.9038706145,94.703755044647806,2.9972803820098551E-2,21848.201207427515,29.999998694086802,9.3929214950983289E-2,9812737.9558368158,0.49692231164839906]
[125.45454545454544,0.52789586008125666,0.94306140283582429,100.68695969778584,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A41,$B$6,$B$7),m_function(D41,$B$6,$B$7))","v":1554430.9304418513},0.94850758785817635,77.370878224903194,0.94288725909207627,0.94569742347512631,0.30703874546426047,40506.781015299654,77.362961873485546,2.933412229398848E-2,21798.407136287435,29.999999679823485,7.4396398258865792E-2,7772154.6522092558,0.39358607899718678]
[100.36363636363635,0.62452185176761266,0.94859995357347315,77.775100207511542,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A42,$B$6,$B$7),m_function(D42,$B$6,$B$7))","v":1142002.8156114165},0.95634694083440175,60.492334309845148,0.95297206521623457,0.95465950302531821,0.30415635058616869,40288.634467810756,60.490730102152149,2.7859058114774897E-2,21741.213651262024,30.000543644308735,5.4656243724554153E-2,5710014.0780570824,0.28915817460765519]
[75.272727272727252,0.72096740372694046,0.95735738065672671,56.2042745247482,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A43,$B$6,$B$7),m_function(D43,$B$6,$B$7))","v":722997.29276040802},0.96599545582391066,44.854273324937466,0.96360463232726457,0.96480004407558762,0.30095951205184379,40045.942928293,44.855183664160208,2.4051997669682024E-2,21681.398541835079,30.000049029072212,3.4603213946970426E-2,3614986.4638020401,0.1830648528733681]
[{"$f":"D44","v":34.810544444014198},0.87362232955042685,0.97753394740862143,34.810544444014198,0,0.97753394740862143,29.999744746756658,0.97474812282265999,0.97614103511564076,0.29746290755842203,39779.577046902559,{"$f":"Tubingp2_noflow(J44,D44)","v":29.999745202328803},0,21619.235992339894,{"$f":"L44","v":29.999745202328803},0,0,0]

{"sheet":"Data_IPR_only","index":3,"n_rows":44,"n_cols":11,"rows_kept":44,"cut":false,"hidden":false,"merged":[]}
["CONFIGURATION: Standalone wells",null,null,null,null,"RESULTS"]
["Reservoir",null,null,null,null,"IPR only, pwf = 30 bara",null,"IPR only, pwf = 60 bara",null,"IPR only, pwf = 90 bara"]
["G",270000000000,"[Sm3]",null,null,"RF","qpp_n","RF","qpp_n","RF","qpp_n"]
["n",1,"[-]",null,null,"[-]","[-]","[-]","[-]","[-]","[-]"]
["pi",276,"[bara]",null,null,0,1,0,1,0,1]
["TR",90,"[C]",null,null,8.623973140273411E-2,0.83120268107258066,7.1482549925782846E-2,0.85254235712045845,7.1482549925782846E-2,0.84114578328415013]
["Sg",0.5,"[-]",null,null,0.17792445132208923,0.67197974408741556,0.1467752084001972,0.71181111265979469,0.1467752084001972,0.68953782882560777]
["Well",null,null,null,null,0.27465683565445265,0.52427654795239909,0.22569850541564007,0.57894042975324655,0.22569850541564007,0.54639795594114682]
["skin",3,"[-]",null,null,0.37567439674215641,0.39021331979596147,0.30790165145435777,0.45515889255966302,0.30790165145435777,0.41304970249840406]
["external radius, re",453.85,"[m]",null,null,0.47985929374878955,0.27201651617199379,0.39285334505258873,0.34180579971625447,0.39285334505258873,0.2909358776445215]
["wellbore radius",0.11,"[m]",null,null,0.58583237782788866,0.17185047700205716,0.47985929374878944,0.24021364842236101,0.47985929374878944,0.18149196342535132]
["kh",{"$f":"1*2030","v":2030},"[md m]",null,null,0.69211548734671191,9.1726719786241556E-2,0.5681088249096764,0.15169160038416196,0.5681088249096764,8.6128302860952397E-2]
["Field",null,null,null,null,0.79731065439449056,3.3317776810955942E-2,0.65674307926382269,7.7481820453129596E-2,0.65674307926382269,6.1830641239556993E-3]
["psep",{"$f":"(1)*30","v":30},"bara",null,null,0.89140267496171133,0,0.77914905162208958,0,0.6644406881095668,0]
["Nw",5,"[-]"]
["Tubing"]
["Tubing TVD",3000,"[m]"]
["Internal Diameter",{"$f":"0.15*1","v":0.15},"[m]"]
["A",{"$f":"0.25*PI()*B18^2","v":1.7671458676442587E-2},"[m2]"]
["L",3000,"[m]"]
["Twh",70,"[C]"]
["Friction factor",{"$f":"ff($B$18)","v":1.1777314787101792E-2},"[-]"]
["Sound speed at wh",{"$f":"SQRT(k_const(B7)*8314*(B21+273.15)/(B7*28.93))","v":509.3698309516567},"[m/s]"]
["Flowline"]
["L",10000,"[m]"]
["Tsep",60,"[C]"]
["Internal Diameter",{"$f":"6*25.4/1000","v":0.15239999999999998},"[m]"]
["A",{"$f":"0.25*PI()*B27^2","v":1.8241469247509915E-2},"[m2]"]
["Friction factor",{"$f":"ff($B$27)","v":1.1735513370070387E-2},"[-]"]
["Zsep",{"$f":"ZfacStanding($B$14,$B$26,$B$7,2)","v":0.97138593747056057},"[-]"]
["Sound speed at sep",{"$f":"SQRT(k_const(B7)*8314*(B26+273.15)/(B7*28.93))","v":501.89298563752271},"[m/s]"]
[]
["pR","RF","ZR","pwf","qwell","qfield","qpp_n"]
["[bara]","[-]","[-]","[bara]","[Sm3/d]","[Sm3/d]","[-]"]
[{"$f":"$B$5","v":276},{"$f":"MBgastank_RF($A$35,$C$35,C35,A35)","v":0},{"$f":"ZfacStanding(A35,$B$6,$B$7,2)","v":0.97949102344801509},30,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A35,$B$6,$B$7),m_function(D35,$B$6,$B$7))","v":18763217.162348043},{"$f":"E35*$B$15","v":93816085.81174022},{"$f":"F35/$F$35","v":1}]
[{"$f":"A35+(-$A$35/12)","v":253},{"$f":"MBgastank_RF($A$35,$C$35,C36,A36)","v":7.1482549925782846E-2},{"$f":"ZfacStanding(A36,$B$6,$B$7,2)","v":0.96698965799969261},30,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A36,$B$6,$B$7),m_function(D36,$B$6,$B$7))","v":16112248.273736715},80561241.368683577,0.85871458686034929]
[{"$f":"A36+(-$A$35/12)","v":230},0.1467752084001972,0.95665588667384094,30,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A37,$B$6,$B$7),m_function(D37,$B$6,$B$7))","v":13582205.453063527},67911027.265317634,0.72387402093915965]
[207,0.22569850541564007,0.94874964432342934,30,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A38,$B$6,$B$7),m_function(D38,$B$6,$B$7))","v":11193478.495848142},55967392.479240708,0.59656499197323054]
[184,0.30790165145435777,0.94349887845303337,30,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A39,$B$6,$B$7),m_function(D39,$B$6,$B$7))","v":8968154.6830110196},44840773.415055096,0.47796465848123976]
[161,0.39285334505258873,0.94107372415236101,30,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A40,$B$6,$B$7),m_function(D40,$B$6,$B$7))","v":6930311.7018830553},34651558.509415276,0.36935625921284121]
[138,0.47985929374878944,0.94156351509907954,30,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A41,$B$6,$B$7),m_function(D41,$B$6,$B$7))","v":5103904.9646804761},25519524.823402382,0.27201651617199368]
[115,0.5681088249096764,0.94496318357200482,30,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A42,$B$6,$B$7),m_function(D42,$B$6,$B$7))","v":3512470.3620188492},17562351.810094245,0.18719979263829484]
[92,0.65674307926382269,0.95117385285567591,30,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A43,$B$6,$B$7),m_function(D43,$B$6,$B$7))","v":2178339.3262435966},10891696.631217983,0.11609625936722875]
[{"$f":"D44","v":30},0.89140267496171133,0.98037788273917637,30,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A44,$B$6,$B$7),m_function(D44,$B$6,$B$7))","v":0},0,0]

{"sheet":"Data_IPR_changing_pwf","index":4,"n_rows":44,"n_cols":11,"rows_kept":44,"cut":false,"hidden":false,"merged":[]}
["CONFIGURATION: Standalone wells",null,null,null,null,"RESULTS"]
["Reservoir",null,null,null,null,"IPR only, pwf = 30 bara",null,"IPR only, pwf = 60 bara",null,"IPR only, pwf = 90 bara"]
["G",270000000000,"[Sm3]",null,null,"RF","qpp_n","RF","qpp_n","RF","qpp_n"]
["n",1,"[-]",null,null,"[-]","[-]","[-]","[-]","[-]","[-]"]
["pi",276,"[bara]",null,null,0,1,0,1,0,1]
["TR",90,"[C]",null,null,8.623973140273411E-2,0.83120268107258066,7.1482549925782846E-2,0.85254235712045845,7.1482549925782846E-2,0.84114578328415013]
["Sg",0.5,"[-]",null,null,0.17792445132208923,0.67197974408741556,0.1467752084001972,0.71181111265979469,0.1467752084001972,0.68953782882560777]
["Well",null,null,null,null,0.27465683565445265,0.52427654795239909,0.22569850541564007,0.57894042975324655,0.22569850541564007,0.54639795594114682]
["skin",3,"[-]",null,null,0.37567439674215641,0.39021331979596147,0.30790165145435777,0.45515889255966302,0.30790165145435777,0.41304970249840406]
["external radius, re",453.85,"[m]",null,null,0.47985929374878955,0.27201651617199379,0.39285334505258873,0.34180579971625447,0.39285334505258873,0.2909358776445215]
["wellbore radius",0.11,"[m]",null,null,0.58583237782788866,0.17185047700205716,0.47985929374878944,0.24021364842236101,0.47985929374878944,0.18149196342535132]
["kh",{"$f":"1*2030","v":2030},"[md m]",null,null,0.69211548734671191,9.1726719786241556E-2,0.5681088249096764,0.15169160038416196,0.5681088249096764,8.6128302860952397E-2]
["Field",null,null,null,null,0.79731065439449056,3.3317776810955942E-2,0.65674307926382269,7.7481820453129596E-2,0.65674307926382269,6.1830641239556993E-3]
["psep",{"$f":"(1)*30","v":30},"bara",null,null,0.89140267496171133,0,0.77914905162208958,0,0.6644406881095668,0]
["Nw",5,"[-]"]
["Tubing"]
["Tubing TVD",3000,"[m]"]
["Internal Diameter",{"$f":"0.15*1","v":0.15},"[m]"]
["A",{"$f":"0.25*PI()*B18^2","v":1.7671458676442587E-2},"[m2]"]
["L",3000,"[m]"]
["Twh",70,"[C]"]
["Friction factor",{"$f":"ff($B$18)","v":1.1777314787101792E-2},"[-]"]
["Sound speed at wh",{"$f":"SQRT(k_const(B7)*8314*(B21+273.15)/(B7*28.93))","v":509.3698309516567},"[m/s]"]
["Flowline",null,null,null,null,null,null,null,"min value",{"$f":"ROW(A35)","v":35}]
["L",10000,"[m]",null,null,null,null,null,"max value",{"$f":"ROW(A44)-1","v":43}]
["Tsep",60,"[C]"]
["Internal Diameter",{"$f":"6*25.4/1000","v":0.15239999999999998},"[m]"]
["A",{"$f":"0.25*PI()*B27^2","v":1.8241469247509915E-2},"[m2]"]
["Friction factor",{"$f":"ff($B$27)","v":1.1735513370070387E-2},"[-]"]
["Zsep",{"$f":"ZfacStanding($B$14,$B$26,$B$7,2)","v":0.97138593747056057},"[-]"]
["Sound speed at sep",{"$f":"SQRT(k_const(B7)*8314*(B26+273.15)/(B7*28.93))","v":501.89298563752271},"[m/s]"]
[]
["pR","RF","ZR","pwf","qwell","qfield","qpp_n","qfield_basecase"]
["[bara]","[-]","[-]","[bara]","[Sm3/d]","[Sm3/d]","[-]","[Sm3/d]"]
[276,{"$f":"MBgastank_RF($A$35,$C$35,C35,A35)","v":0},{"$f":"ZfacStanding(A35,$B$6,$B$7,2)","v":0.97949102344801509},241.34478056511438,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A35,$B$6,$B$7),m_function(D35,$B$6,$B$7))","v":3949405.4719576789},{"$f":"E35*$B$15","v":19747027.359788395},{"$f":"F35/$F$35","v":1},19747027.359788384]
[250.90909090909091,{"$f":"MBgastank_RF($A$35,$C$35,C36,A36)","v":7.8171458235153368E-2},{"$f":"ZfacStanding(A36,$B$6,$B$7,2)","v":0.96595662274458938},218.00832642794987,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A36,$B$6,$B$7),m_function(D36,$B$6,$B$7))","v":3559215.1840002323},17796075.92000116,0.90120277830981133,17796075.920001104]
[225.81818181818181,0.1608627327821176,0.9550305745739005,194.59389609195765,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A37,$B$6,$B$7),m_function(D37,$B$6,$B$7))","v":3165347.1918331254},15826735.959165627,0.80147435210396256,15826735.959165443]
[200.72727272727272,0.24781137811331766,0.94704584360159316,171.10925150760568,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A38,$B$6,$B$7),m_function(D38,$B$6,$B$7))","v":2767908.4683381277},13839542.341690639,0.70084180720145317,13839542.341690602]
[175.63636363636363,0.33850852012316635,0.94228344344355919,147.57682133359896,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A39,$B$6,$B$7),m_function(D39,$B$6,$B$7))","v":2366941.12406016},11834705.6203008,0.59931580610458113,11834705.620119866]
[150.54545454545453,0.43219357131538294,0.94093304334248529,124.06142052743121,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A40,$B$6,$B$7),m_function(D40,$B$6,$B$7))","v":1962555.1418242201},9812775.7091211006,0.49692419675800015,9812775.7091212254]
[125.45454545454544,0.52789586008125666,0.94306140283582429,100.68684389384275,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A41,$B$6,$B$7),m_function(D41,$B$6,$B$7))","v":1554437.4852136627},7772187.4260683134,0.39358771750603372,7772187.4260682994]
[100.36363636363635,0.62452185176761266,0.94859995357347315,77.774931418971079,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A42,$B$6,$B$7),m_function(D42,$B$6,$B$7))","v":1142010.3333018192},5710051.6665090956,0.28916006254879079,5710051.6667251429]
[75.272727272727252,0.72096740372694046,0.95735738065672671,56.204244251927285,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A43,$B$6,$B$7),m_function(D43,$B$6,$B$7))","v":722998.27921874821},3614991.3960937411,0.18306509279746491,3614991.396093695]
[34.810841610496745,0.87362122834455058,0.97753377445405087,34.799999999999997,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A44,$B$6,$B$7),m_function(D44,$B$6,$B$7))","v":220.35317649904857},1101.7658824952427,5.5794012051596661E-5,0]

{"sheet":"Data_Network","index":5,"n_rows":52,"n_cols":23,"rows_kept":52,"cut":false,"hidden":false,"merged":[]}
["CONFIGURATION: Wells on network",null,null,null,null,"RESULTS"]
["Reservoir",null,null,null,"NAME","network: 4 wells, 1 template",null,"network: 16 wells, 4 templates",null,"network: 16 wells, 16 templates"]
["G",270000000000,"[Sm3]",null,"ID flowline[m]",0.20319999999999999,null,0.20319999999999999,null,0.15240000000000001]
["n",1,"[-]",null,"ID pipeline [m]",0.254,null,0.50800000000000001,null,0.50800000000000001]
["pi",276,"[bara]",null,null,"RF","qpp_n","RF","qpp_n","RF","qpp_n"]
["TR",90,"[C]",null,null,"[-]","[-]","[-]","[-]","[-]","[-]"]
["Sg",0.5,"[-]",null,null,0,1,0,1,0,1]
["Well",null,null,null,null,7.8171458235153368E-2,0.90276573785683933,7.8171458235153368E-2,0.90371256555331514,7.8171458235153368E-2,0.90346713130440059]
["skin",3,"[-]",null,null,0.1608627327821176,0.80551903931598701,0.1608627327821176,0.80676496767320172,0.1608627327821176,0.80618105234874482]
["external radius, re",453.85,"[m]",null,null,0.24781137811331755,0.708242337442064,0.24781137811331755,0.70924873365493069,0.24781137811331755,0.70819136560521945]
["wellbore radius",0.11,"[m]",null,null,0.33850852012316635,0.61081271209315291,0.33850852012316635,0.61115540586193529,0.33850852012316635,0.60951364622511028]
["kh",{"$f":"1*2030","v":2030},"[md m]",null,null,0.43219357131538294,0.51312777373331464,0.43219357131538294,0.51247443245193836,0.43219357131538294,0.510140696697718]
["Field",null,null,null,null,0.52789586008125666,0.41491894453241501,0.52789586008125666,0.41300103880650157,0.52789586008125666,0.40990260761916708]
["psep",{"$f":"(1)*30","v":30},"bara",null,null,0.62452185176761266,0.31575720865168483,0.62452185176761266,0.31230568230312122,0.62452185176761266,0.30846674784553874]
["Nwells per template",1,"[-]",null,null,0.72096740372694046,0.21448628972616565,0.72096740372694046,0.20915044464087137,0.72096740372694046,0.20492756957811253]
["Ntemplates",16,"[-]",null,null,0.87362122834455058,0,0.87362122834455058,0,0.87362122834455058,0]
["Tubing"]
["Tubing TVD",3000,"[m]",null,null,"Deviation against base case"]
["Internal Diameter",{"$f":"0.15*1","v":0.15},"[m]",null,null,"at RF = 0.721"]
["A",{"$f":"0.25*PI()*B19^2","v":1.7671458676442587E-2},"[m2]",null,null,"max dev  (net)","[%]",{"$f":"ABS(K15-Data_Standalone!G13)*100/Data_Standalone!G13","v":11.868345251294745}]
["L",3000,"[m]",null,null,null,null,null,null,null,null,null,"Instructions to solve"]
["Twh",70,"[C]",null,null,null,null,null,null,null,null,null,{"$f":"\"1. Provide a suitable seed in column D (e.g. 5 bara less than pR)\"","v":"1. Provide a suitable seed in column D (e.g. 5 bara less than pR)"}]
["Friction factor",{"$f":"ff($B$19)","v":1.1777314787101792E-2},"[-]",null,null,null,null,null,null,null,null,null,{"$f":"\"2. click solve all to find maximum rates\"","v":"2. click solve all to find maximum rates"}]
["Sound speed at wh",{"$f":"SQRT(k_const(B7)*8314*(B22+273.15)/(B7*28.93))","v":509.3698309516567},"[m/s]",null,null,null,null,null,"From:",{"$f":"ROW(A43)","v":43},null,null,{"$f":"\"3. copy column L to G  and Q to N (values only). If psep, pwh or ppipeline_in change significantly, repeat from step 2.\"","v":"3. copy column L to G  and Q to N (values only). If psep, pwh or ppipeline_in change significantly, repeat from step 2."}]
["Flowline",null,null,null,null,null,null,null,"To:",{"$f":"ROW(A52)","v":52}]
["L",5000,"[m]"]
["ID",{"$f":"6*25.4/1000","v":0.15239999999999998},"[m]"]
["Area",{"$f":"0.25*PI()*B27^2","v":1.8241469247509915E-2},"[m2]"]
["Friction factor",{"$f":"ff($B$27)","v":1.1735513370070387E-2},"[-]"]
["Pipeline"]
["L",60000,"[m]"]
["Tin",60,"[C]"]
["Sound speed at pipein",{"$f":"SQRT(k_const(B7)*8314*(B32+273.15)/(B7*28.93))","v":501.89298563752271},"[m/s]"]
["Tsep",30,"[C]"]
["Internal Diameter",{"$f":"20*25.4/1000","v":0.50800000000000001},"[m]"]
["A",{"$f":"0.25*PI()*B35^2","v":0.20268299163899911},"[m2]"]
["Friction factor",{"$f":"ff($B$35)","v":8.9614286972534672E-3},"[-]"]
["Zsep",{"$f":"ZfacStanding($B$14,$B$34,$B$7,2)","v":0.958328110569169},"[-]"]
["Sound speed at sep",{"$f":"SQRT(k_const(B7)*8314*(B34+273.15)/(B7*28.93))","v":478.76236493424193},"[m/s]"]
[null,null,null,"Guess (solver)",null,null,"Guess (manual)",null,null,null,null,"2. Paste to G",{"$f":"MAX(M43:M52)","v":1.7580719131646744E-2},"Guess (manual)",null,null,"3. Paste to N",{"$f":"MAX(R43:R52)","v":1.7858948043326547E-2},null,null,{"$f":"MAX(U43:U52)","v":0.16597228217949023}]
["pR","RF","ZR","pwf","qwell","Zwf","pwh","Zwh","Zav_Tub","S","CT","pwh","Mch at wh","ppipeline_in","Z_pipeline_in","Cflow","ppipeline_in","Mch at pipein","Cpipelines","psep","Mch at sep","qfield","qpp_n"]
["[bara]","[-]","[-]","[bara]","[Sm3/d]","[-]","[bara]","[-]","[-]","[-]","Sm3/bar","[bara]","[-]","[bara]","[-]","Sm3/bar ","[bara]","[-]","Sm3/bar ","[bara]","[-]","[Sm3/d]","[-]"]
[{"$f":"$B$5","v":276},{"$f":"MBgastank_RF($A$43,$C$43,C43,A43)","v":0},{"$f":"ZfacStanding(A43,$B$6,$B$7,2)","v":0.97949102344801509},253.815402148331,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A43,$B$6,$B$7),m_function(D43,$B$6,$B$7))","v":2558956.7582492959},{"$f":"ZfacStanding(D43,$B$6,$B$7,2)","v":0.96739738370208239},208.58764649152101,{"$f":"ZfacStanding(G43,$B$22,$B$7,2)","v":0.92542844534484148},{"$f":"(H43+F43)*0.5","v":0.94641291452346188},{"$f":"s($B$7,(($B$22+$B$6)*0.5)+273.15,I43,$B$18)","v":0.30680662323674157},{"$f":"Cflowconst($B$19,$B$7,$B$23,I43,(($B$22+$B$6)*0.5)+273.15,$B$21,J43)","v":40489.236824288339},{"$f":"Tubingp2(K43,J43,D43,E43)","v":208.34366573216192},{"$f":"(Bg(G43,$B$22,H43,2)*E43/($B$20*24*3600))/$B$24","v":1.7580719131646744E-2},191.00605594474837,{"$f":"ZfacStanding(N43,$B$32,$B$7,2)","v":0.90713050725031341},{"$f":"Cflowconst($B$27,$B$7,$B$29,(H43+O43)*0.5,(($B$32+$B$22)*0.5)+273.15,$B$26,0)","v":31507.412550933757},{"$f":"linep2(P43,G43,E43*$B$15)","v":192.12627624756709},{"$f":"(Bg(Q43,$B$32,O43,2)*E43*$B$15/($B$28*24*3600))/$B$33","v":1.7858948043326547E-2},{"$f":"Cflowconst($B$35,$B$7,$B$37,(O43+$B$38)*0.5,(($B$34+$B$32)*0.5)+273.15,$B$31,0)","v":215752.7295976826},{"$f":"linep2(S43,Q43,V43)","v":30.00011349952468},{"$f":"(Bg(T43,$B$34,$B$38,2)*V43/($B$36*24*3600))/$B$39","v":0.16597228217949023},{"$f":"E43*$B$15*$B$16","v":40943308.131988734},{"$f":"V43/$V$43","v":1}]
[{"$f":"A43+(-$A$43/11)","v":250.90909090909091},7.8171458235153368E-2,{"$f":"ZfacStanding(A44,$B$6,$B$7,2)","v":0.96595662274458938},229.83988300157282,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A44,$B$6,$B$7),m_function(D44,$B$6,$B$7))","v":2311933.3215075},{"$f":"ZfacStanding(D44,$B$6,$B$7,2)","v":0.95659216672004832},188.74938559539825,0.92072191697485373,{"$f":"(H44+F44)*0.5","v":0.93865704184745102},0.30934168449968974,40680.621496715314,{"$f":"Tubingp2(K44,J44,D44,E44)","v":188.52336197883668},1.7463756493114008E-2,172.92041607636932,0.9050232915514963,31566.151173328082,{"$f":"linep2(P44,G44,E44*$B$15)","v":173.9600561326051},{"$f":"(Bg(Q44,$B$32,O44,2)*E44*$B$15/($B$28*24*3600))/$B$33","v":1.7778513298639949E-2},215874.68970583365,30.000009703141291,0.1499510204672394,36990933.14412,0.90346713130440059]
[225.81818181818181,0.1608627327821176,0.9550305745739005,205.80677991734953,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A45,$B$6,$B$7),m_function(D45,$B$6,$B$7))","v":2062982.45228035},0.94841017639572123,168.96977182416211,0.91858606102500184,0.93349811871036148,0.3110512433530449,40809.414062388023,168.75451623004361,1.7367039629566809E-2,154.85418689929909,0.90539604227236115,31581.403791036009,155.83237507994431,1.7716843751336381E-2,215853.10081621178,29.999391693888487,0.133806928515843,33007719.2364856,0.80618105234874482]
[200.72727272727272,0.24781137811331766,0.94704584360159316,181.71641659596261,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A46,$B$6,$B$7),m_function(D46,$B$6,$B$7))","v":1812231.0811492743},0.94312959242166006,149.23679878581464,0.91910068609361284,0.93111513925763645,0.31184730894193208,40869.313357112798,149.02391079675979,1.7283041323841779E-2,136.80352840068639,0.90828295295396066,31551.996908617461,137.74138620069323,1.766364012274103E-2,215686.11644481914,30.000037163562919,0.11754043625358473,28995697.298388388,0.70819136560521945]
[175.63636363636363,0.33850852012316635,0.94228344344355919,157.57502081261734,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A47,$B$6,$B$7),m_function(D47,$B$6,$B$7))","v":1559719.0642529165},0.94096097382382049,129.54012807896845,0.92227397331400218,0.93161747356891134,0.31167915880777863,40856.664922007483,129.3193361212812,1.7195762547364445E-2,118.7705091760357,0.91364624597978117,31478.556903113324,119.6895108477645,1.7598606547828365E-2,215376.91947538269,29.999289122613717,0.10116515081349081,24955505.028046664,0.60951364622511028]
[150.54545454545453,0.43219357131538294,0.94093304334248529,133.4140835435322,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A48,$B$6,$B$7),m_function(D48,$B$6,$B$7))","v":1305427.9834726297},0.94201097591129257,109.89075702928983,0.92803214573811854,0.93502156082470556,0.31054444374146678,40771.256013531514,109.64750572733521,1.7071598993502725E-2,100.77726274727272,0.92136948408140396,31363.613897874446,101.70327765855812,1.7480816431153425E-2,214933.99732860629,30.00000781352578,8.466951394183217E-2,20886847.735562075,0.510140696697718]
[125.45454545454544,0.52789586008125666,0.94306140283582429,109.28553679130613,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A49,$B$6,$B$7),m_function(D49,$B$6,$B$7))","v":1048923.0479910769},0.94624953959288527,90.324434786109151,0.93621333694023501,0.94123143826656008,0.30849559278145749,40616.799313637996,90.033676686850811,1.6835756171534589E-2,82.871529394820953,0.93125549474185709,31211.528370958295,83.839603231467308,1.7221587457181848E-2,214371.00919575428,30.000025227349536,6.8032671436849546E-2,16782768.767857231,0.40990260761916708]
[100.36363636363635,0.62452185176761266,0.94859995357347315,85.346402856315592,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A50,$B$6,$B$7),m_function(D50,$B$6,$B$7))","v":789353.06909452274},0.95347108024177074,70.9904230179569,0.94652109094575865,0.94999608559376469,0.30564941781955074,40401.712372649657,70.597512784141756,1.6297510198904727E-2,65.207138668980107,0.94297624413538672,31029.056841233782,66.275858483346241,1.6600708025361236E-2,213709.23373687119,29.999879914980877,5.1197328745057225E-2,12629649.105512364,0.30846674784553874]
[75.272727272727252,0.72096740372694046,0.95735738065672671,62.007965837434959,{"$f":"iprppgas_qg($B$12,$B$6+273.15,$B$10,$B$11,$B$9,m_function(A51,$B$6,$B$7),m_function(D51,$B$6,$B$7))","v":524400.78912351385},0.963194861219835,52.357182070294641,0.95835610328006204,0.96077548224994858,0.30222019176905551,40141.743573718712,51.686158784877058,1.486392185304178E-2,48.208335259649481,0.95591712542829954,30827.602751429546,49.516752095355443,1.4963781131297451E-2,212985.63895137477,30.000010855369013,3.4012412776448391E-2,8390412.6259762216,0.20492756957811253]
[{"$f":"D52","v":34.810841610496745},0.87362122834455058,0.97753377445405087,34.810841610496745,0,0.97753377445405087,30.000000448095001,0.97474792279041167,0.97614084862223127,0.2974629643892287,39779.581384078934,{"$f":"Tubingp2_noflow(J52,D52)","v":30.000000448095001},0,30.000000448095001,0.9713859370710497,30574.218322926437,30.000000448095001,0,212130.26250950291,30.000000448095001,0,0,0]