{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Input","Annulus_h","Internal h"],"not_rendered":{"charts":0,"images":3,"macros":1,"external_links":0,"defined_names":27,"comments":4,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Input","index":0,"n_rows":20,"n_cols":15,"rows_kept":20,"cut":false,"hidden":false,"merged":[]}
["Layer nr","TAG","Type","ID","OD","k","alpha","h","ref D for h"]
["[-]","[-]","[SOLID, STILLFLUID, SOIL, HEXT]","[m]","[m]","[W/m K]","[m2/d]","[W/m2 K]"]
[1,"prod fluid","FLUID",null,null,null,null,5000,0.15]
[2,"tubing","SOLID",{"$f":"6.1*25.4/1000","v":0.15493999999999997},{"$f":"7*25.4/1000","v":0.17779999999999999},55]
[3,"prod casing","SOLID",{"$f":"0.1118616*2","v":0.22372320000000001},{"$f":"(9+(5/8))*25.4/1000","v":0.244475},55]
[4,"surface casing","SOLID",{"$f":"0.1575816*2","v":0.31516319999999998},{"$f":"2*0.1697736","v":0.33954719999999999},55]
[5,"annulus","FLUID",null,null,null,null,100,{"$f":"7*25.4/1000","v":0.17779999999999999}]
[6,"cement","SOLID",{"$f":"E5","v":0.244475},{"$f":"0.155448*2","v":0.31089600000000001},1.7]
[7,"cement","SOLID",{"$f":"E6","v":0.33954719999999999},{"$f":"0.2221992*2","v":0.44439840000000003},1.7]
[8,"formation","SOIL",{"$f":"0.155448*2","v":0.31089600000000001},null,2.98,{"$f":"1.12*0.09290304","v":0.10405140480000001}]
[9,"formation","SOIL",{"$f":"0.2221992*2","v":0.44439840000000003},null,2.98,{"$f":"1.12*0.09290304","v":0.10405140480000001}]
[]
[]
[null,null,null,"ref D"]
[null,null,null,"[m]","t [d]","LAYER Nr. 1","LAYER Nr. 2","LAYER Nr. 3","LAYER Nr. 4","LAYER Nr. 5","LAYER Nr. 6","LAYER Nr. 7","LAYER Nr. 8",null,"U [W/m2 K]"]
[null,null,null,0.15,1.1731385997537029,1,2,5,3,6,4,7,9,null,{"$f":"Ucalc(F16:N16,A3:I11,D16,E16)","v":9.0004115639193021}]
[]
[null,null,null,"Tf","Tform","d","dQ/dL","Tdist"]
[null,null,null,"[C]","[C]","[m]","[W/m]","[C]"]
[null,null,null,90.927220341104842,65.714285714285722,0.15,{"$f":"dqdl(O16,F20,D20,E20)","v":-106.93672968950972},{"$f":"tcalc(F16:N16,A3:I11,G20,D20,E20)","v":"90.9272203411048,90.8818349834297,90.8392486507571,88.9247931807721,88.8973442771287,86.4911321144061,86.4680714947971,83.7738982962993,65.7142857142857"}]

{"sheet":"Annulus_h","index":1,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[]}
["Tinner","[C]",61.182809983918801,null,"Based on SPE1449, by Willhite"]
["Touter","[C]",59.820754126352902]
["rin","[m]",8.8899999999999993E-2]
["rout","[m]",0.11186160000000001]
["den","[kg/m3]",1000]
["visc","[cP]",1]
["visc","[Pa s]",{"$f":"C6*0.001","v":1E-3}]
["Cp","[J/kg C]",4200]
["k","[W/m K]",0.59799999999999998]
["beta","[1/C]",2.1000000000000001E-4]
[]
["hc","[W/m2 K]",{"$f":"hccalc(C3,C4,C5,C10,C2,C1,C7,C8,C9)","v":102.7846354138814}]

{"sheet":"Internal h","index":2,"n_rows":14,"n_cols":3,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
["Tf","[C]",61.382631408739101]
["Tw","[C]",61.304003638779598]
["D","[m]",0.154]
["den","[kg/m3]",750]
["visc","[cP]",1]
["visc","[Pa s]",{"$f":"C5*0.001","v":1E-3}]
["Cp","[J/kg C]",4200]
["k","[W/m K]",0.59799999999999998]
["beta","[1/C]",2.1000000000000001E-4]
["teta","[rad]",0]
["V","[m/s]",2]
[]
[]
["h","[W/m2 K]",{"$f":"h_in(C8,C3,C7,C9,C2,C1,C6,C10,C11,C4)","v":4352.9221275253094}]