{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Data","rel_perm","PVT"],"not_rendered":{"charts":4,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Data","index":0,"n_rows":38,"n_cols":10,"rows_kept":38,"cut":false,"hidden":false,"merged":[]}
["Prof. Milan Stanko (NTNU)"]
["Rp","[Sm3/Sm3]",300]
[]
["COLUMN",4,6,3,5,2]
["p","Rs","viscg","Bg","Visco","Bo","krg/kro","kro","kro/(visco*Bo)","So"]
["[bara]","[Sm3/Sm3]","[cp]","[m3/Sm3]","[cp]","[m3/Sm3]","[-]","[-]","[1/cp]","[-]"]
[1.01325]
[5]
[50]
[100]
[150]
[200]
[250]
[300]
[330]
[360]
[382.91]
[]
["IPR"]
["permeability, k","[md]",100]
["layer height, h","[m]",50]
["external res radius, re","[m]",500]
["wellbore radius, rw","[m]",0.15]
["Skin, s","[-]",0]
["pR","[bara]",382]
[]
[]
["pwf","m(p)","qo","qo - fet","qo -Vogel"]
["[bara]","[bara/cp]","[Sm3/d]","[Sm3/d]","[Sm3/d]"]
[{"$f":"C25","v":382}]
[300]
[250]
[200]
[150]
[100]
[50]
[5]
[1.01325]

{"sheet":"rel_perm","index":1,"n_rows":52,"n_cols":6,"rows_kept":52,"cut":false,"hidden":false,"merged":[]}
["Connate water saturation, Swc","[-]",0.3]
["Residual oil saturation to gas,  [Sorg]","[-]",0]
[]
["Sg","kro","krg","krg/kro","kro","So"]
[0,1,0]
[1.489E-2,0.89805000000000001,1.289E-3]
[2.9790000000000001E-2,0.80459000000000003,3.2190000000000001E-3]
[4.4679999999999997E-2,0.71906999999999999,5.8719999999999996E-3]
[5.9569999999999998E-2,0.64098999999999995,9.3189999999999992E-3]
[7.4469999999999995E-2,0.56984000000000001,1.3622E-2]
[8.9359999999999995E-2,0.50516000000000005,1.8835000000000001E-2]
[0.10426000000000001,0.44649,2.5003999999999998E-2]
[0.11915000000000001,0.39340000000000003,3.2167000000000001E-2]
[0.13403999999999999,0.34548000000000001,4.0353E-2]
[0.14893999999999999,0.30236000000000002,4.9586999999999999E-2]
[0.16383,0.26365,5.9886000000000002E-2]
[0.17871999999999999,0.22900999999999999,7.1258000000000002E-2]
[0.19361999999999999,0.19811000000000001,8.3710000000000007E-2]
[0.20851,0.17063999999999999,9.7240999999999994E-2]
[0.22339999999999999,0.14630000000000001,0.11183999999999999]
[0.23830000000000001,0.12483,0.12751000000000001]
[0.25319000000000003,0.10595,0.14421999999999999]
[0.26808999999999999,8.9432999999999999E-2,0.16197]
[0.28298000000000001,7.5040999999999997E-2,0.18071999999999999]
[0.29787000000000002,6.2564999999999996E-2,0.20044999999999999]
[0.31276999999999999,5.1805999999999998E-2,0.22115000000000001]
[0.32766000000000001,4.258E-2,0.24276]
[0.34255000000000002,3.4719E-2,0.26527000000000001]
[0.35744999999999999,2.8063999999999999E-2,0.28865000000000002]
[0.37234,2.2471000000000001E-2,0.31285000000000002]
[0.38723000000000002,1.7808000000000001E-2,0.33784999999999998]
[0.40212999999999999,1.3953E-2,0.36359999999999998]
[0.41702,1.0796E-2,0.39007999999999998]
[0.43191000000000002,8.2389999999999998E-3,0.41725000000000001]
[0.44680999999999998,6.1910000000000003E-3,0.44507999999999998]
[0.4617,4.5719999999999997E-3,0.47353000000000001]
[0.47660000000000002,3.3110000000000001E-3,0.50258999999999998]
[0.49148999999999998,2.3449999999999999E-3,0.53220999999999996]
[0.50638000000000005,1.619E-3,0.56237000000000004]
[0.52127999999999997,1.085E-3,0.59306000000000003]
[0.53617000000000004,7.0200000000000004E-4,0.62426000000000004]
[0.55105999999999999,4.3600000000000003E-4,0.65593999999999997]
[0.56596000000000002,2.5740000000000002E-4,0.68810000000000004]
[0.58084999999999998,1.429E-4,0.72074000000000005]
[0.59574000000000005,7.326E-5,0.75385000000000002]
[0.61063999999999996,3.3909999999999999E-5,0.78742999999999996]
[0.62553000000000003,1.363E-5,0.82150000000000001]
[0.64043000000000005,4.4660000000000001E-6,0.85607999999999995]
[0.65532000000000001,1.06E-6,0.89117999999999997]
[0.67020999999999997,1.395E-7,0.92684999999999995]
[0.68511,4.3599999999999998E-9,0.96309999999999996]
[0.7,1E-10,1]

{"sheet":"PVT","index":2,"n_rows":16,"n_cols":6,"rows_kept":16,"cut":false,"hidden":false,"merged":[]}
["p","Bo","Bg","Rs","muo","mug"]
["[bara]","[m^3/Sm^3]","[m^3/Sm^3]","[Sm^3/Sm^3]","[cp]","[cp]"]
[1,{"$f":"0.000005*A3^2 + 0.000005*A3 + 1.1513","v":1.1513100000000001},{"$f":"-0.000000000708*A3^3+ 0.000000652*A3^2 - 0.000205*A3 + 0.0268","v":2.6595651292000002E-2},{"$f":"0.00000339*A3^3- 0.000723*A3^2 + 0.539*A3","v":0.53828039000000005},{"$f":"0.00000675*A3^2 - 0.00576*A3 + 1.41","v":1.40424675},{"$f":"0.0000000754*A3^2+ 0.0000362*A3 + 0.0112","v":1.1236275400000001E-2}]
[30,{"$f":"0.000005*A4^2 + 0.000005*A4 + 1.1513","v":1.15595},{"$f":"-0.000000000708*A4^3+ 0.000000652*A4^2 - 0.000205*A4 + 0.0268","v":2.1217684000000001E-2},{"$f":"0.00000339*A4^3- 0.000723*A4^2 + 0.539*A4","v":15.610830000000002},{"$f":"0.00000675*A4^2 - 0.00576*A4 + 1.41","v":1.2432749999999999},{"$f":"0.0000000754*A4^2+ 0.0000362*A4 + 0.0112","v":1.2353859999999999E-2}]
[40,{"$f":"0.000005*A5^2 + 0.000005*A5 + 1.1513","v":1.1595},{"$f":"-0.000000000708*A5^3+ 0.000000652*A5^2 - 0.000205*A5 + 0.0268","v":1.9597888000000001E-2},{"$f":"0.00000339*A5^3- 0.000723*A5^2 + 0.539*A5","v":20.620160000000002},{"$f":"0.00000675*A5^2 - 0.00576*A5 + 1.41","v":1.1903999999999999},{"$f":"0.0000000754*A5^2+ 0.0000362*A5 + 0.0112","v":1.276864E-2}]
[60,{"$f":"0.000005*A6^2 + 0.000005*A6 + 1.1513","v":1.1696},{"$f":"-0.000000000708*A6^3+ 0.000000652*A6^2 - 0.000205*A6 + 0.0268","v":1.6694272E-2},{"$f":"0.00000339*A6^3- 0.000723*A6^2 + 0.539*A6","v":30.469440000000002},{"$f":"0.00000675*A6^2 - 0.00576*A6 + 1.41","v":1.0886999999999998},{"$f":"0.0000000754*A6^2+ 0.0000362*A6 + 0.0112","v":1.364344E-2}]
[97.54,1.1879999999999999,1.2463E-2,47.5,0.9244,1.5689999999999999E-2]
[132.01,1.2390000000000001,9.1450000000000004E-3,66,0.7611,1.721E-2]
[166.49,1.294,7.3270000000000002E-3,85.9,0.62739999999999996,1.9140000000000001E-2]
[200.96,1.355,6.221E-3,107.8,0.5181,2.1420000000000002E-2]
[235.44,1.4219999999999999,5.4980000000000003E-3,132.19999999999999,0.42799999999999999,2.3949999999999999E-2]
[269.91000000000003,1.4990000000000001,5.0010000000000002E-3,159.9,0.35349999999999998,2.6619999999999998E-2]
[304.38,1.589,4.6439999999999997E-3,192,0.29139999999999999,2.9390000000000003E-2]
[338.86,1.696,4.3819999999999996E-3,230.2,0.2394,3.2250000000000001E-2]
[365.4,1.7949999999999999,4.2259999999999997E-3,265.5,0.2051,3.456E-2]
[382.91,1.8720000000000001,4.1390000000000003E-3,292.60000000000002,0.18459999999999999,3.5959999999999999E-2]