{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Multiphase","Info"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Multiphase","index":0,"n_rows":18,"n_cols":6,"rows_kept":18,"cut":false,"hidden":false,"merged":[]}
["FLUID PROPERTIES","Input:","red"]
[null,"Output:","blue"]
["μo","[Pa s]",3.6624311132707439E-4]
["μg","[Pa s]",0]
["σog","[N/m]",0]
["ρo","[kg/m^3]",610.14309187250115]
["ρg","[kg/m^3]",0,null,"dp/dx","Flow pattern"]
[null,null,null,null,"[Pa/m]","[-]"]
["OPERATING CONDITIONS",null,null,null,{"$f":"multiphasedpdx($C$11,$C$12,$C$7,$C$6,$C$4,$C$3,$C$17,$C$16,$C$5,$C$18)","v":6924.2035449652785},"Liquid"]
[]
["Usl","[m/s]",6.6319069497839003]
["Usg","[m/s]",0]
[]
["PIPING CHARACTERISTICS"]
[]
["Angle (from hor.)","[rad]",{"$f":"90*PI()/180","v":1.5707963267948966}]
["Diameter","[m]",0.15]
["Roughness","[m]",1.5E-5]

{"sheet":"Info","index":1,"n_rows":8,"n_cols":1,"rows_kept":8,"cut":false,"hidden":false,"merged":[]}
["Authors and contributors:"]
[{"$f":"\"-Bushan Yatindra (1997) made the initial version, Synnove Ereiksen (2002) made some modifications and included the slug flow model of Gomez. Andrea Shmueli and Milan Stanko created wrapper functions (2010) . All work supervised by Michael Golan\"","v":"-Bushan Yatindra (1997) made the initial version, Synnove Ereiksen (2002) made some modifications and included the slug flow model of Gomez. Andrea Shmueli and Milan Stanko created wrapper functions (2010) . All work supervised by Michael Golan"}]
["References"]
[{"$f":"\"-D. Barnea, 1986, “A Unified Model for Predicting Flow-Pattern Transitions for the whole Range of Pipe Inclinations”, Int. J. Multiphase Flow\"","v":"-D. Barnea, 1986, “A Unified Model for Predicting Flow-Pattern Transitions for the whole Range of Pipe Inclinations”, Int. J. Multiphase Flow"}]
[{"$f":"\"-L.E. Gomez et al., 1999, A. Unified Mechanistic Model for Steady-State Two-Phase Flow in Wellbores and Pipelines, SPE\"","v":"-L.E. Gomez et al., 1999, A. Unified Mechanistic Model for Steady-State Two-Phase Flow in Wellbores and Pipelines, SPE"}]
[{"$f":"\"-Contact: milanstanko@gmail.com\"","v":"-Contact: milanstanko@gmail.com"}]
["-The author of disclaims any warranty, expressed or implied, as to the accuracy or reliability of the data or calculations contained therein."]
[{"$f":"\"-The tool is not a substitute for sound professional judgment.\"","v":"-The tool is not a substitute for sound professional judgment."}]