{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":1,"images":0,"macros":1,"external_links":0,"defined_names":30,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":18,"n_cols":10,"rows_kept":18,"cut":false,"hidden":false,"merged":[]}
["Prof Milan Stanko (NTNU)",null,null,null,null,null,null,"Example of how to obtain the coefficients if data points are available:"]
["Well data",null,null,null,null,null,null,null,"Plot data points"]
[null,"Units","Well 1","Well 2",null,null,null,null,"Add trendline"]
["a","[(1/1e03 Sm3/d)^3]",-3.9000000000000002E-7,-1.3E-7,null,null,null,null,"select polynomial and increase order"]
["b","[(1/1e03 Sm3/d)^2]",2.1000000000000001E-4,1E-4,null,null,null,null,"Select \"show equation on plot\""]
["c","[(1/1e03 Sm3/d)]",-4.2999999999999997E-2,-2.8000000000000001E-2]
["d","[-]",3.7,3.1,null,null,null,null,"qgi","qo"]
["e","[1e03 Sm3/d]",12,-17,null,null,null,null,50,100]
[null,null,null,null,null,null,null,null,110,170]
["Oil price","[USD/Sm3]",{"$f":"6.29*80","v":503.2},null,null,null,null,null,170,160]
["Gas cost","[USD/Sm3]",{"$f":"2/8","v":0.25}]
[]
[null,null,"Well 1","Well 2","Total","Constraint"]
["qgi","[1E03 Sm3/d]",83.747818234351286,98.311467871295278,{"$f":"C14+D14","v":182.05928610564655},1000]
["qo","[Sm3/d]",{"$f":"qo_GLPerf(C4,C5,C6,C7,C8,C14)","v":124.44327837392001},{"$f":"D4*D14^4+D5*D14^3+D6*D14^2+D7*D14+D8","v":100.01700188580313},{"$f":"C15+D15","v":224.46028025972313}]
["oil revenue","[USD/d]"]
["Gas cost ","[USD/d]"]
["Profit","[USD/d]"]