{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Data"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":28,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Data","index":0,"n_rows":17,"n_cols":10,"rows_kept":17,"cut":false,"hidden":false,"merged":[]}
["Problem 2, Re-sit examination, Prof. Milan Stanko (NTNU)"]
[]
["GOR","[Sm3/Sm3]",150]
["pin,pipeline","[bara]",120]
["uptime","[d/year]",365]
["deno,sc","[kg/m3]",800]
["deng,sc","[kg/m3]",0.8]
["hadia,MPP","[-]",0.6]
[]
["time (end of year)","qo target","Np","pinlet,subseastation","qo avail","pin,pipe","Dpchoke\nDpMPP","mass flow","Dhs","Power, MPP"]
["[years]","[sm3/d]","[Sm3]","[bara]","[sm3/d]","[bara]","[bar]","[kg/s]","[kJ/kg]","[kW]"]
[0,2531,0,129.9608826809382,{"$f":"qo_available(C12,D12)","v":2530.9999999959737},{"$f":"$C$4","v":120},{"$f":"D12-F12","v":9.9608826809381981}]
[1,2531,{"$f":"C12+B12*(A13-A12)*$C$5","v":923815},120.29188201583494,{"$f":"qo_available(C13,D13)","v":2531.000000010622},{"$f":"$C$4","v":120},{"$f":"D13-F13","v":0.29188201583494333}]
[2,2531,{"$f":"C13+B13*(A14-A13)*$C$5","v":1847630},109.6027511168039,{"$f":"qo_available(C14,D14)","v":2531.0000000028936},120,-10.397248883196099,{"$f":"(B14*$C$6+$C$3*B14*$C$7)/(24*3600)","v":26.950462962962963},{"$f":"deltah_s(D14,G14*-1)","v":4.0454540777996435},{"$f":"I14*H14/$C$8","v":181.71143382017797}]
[3,2487,2771445,100.28621560326901,{"$f":"qo_available(C15,D15)","v":2486.9999999959032},120,-19.713784396730986,26.481944444444444,{"$f":"deltah_s(D15,G15*-1)","v":7.904855475370856},348.89323923355585]
[4,2436,3679200,91.582710208442819,{"$f":"qo_available(C16,D16)","v":2436.0000000007681},120,-28.417289791557181,25.93888888888889,{"$f":"deltah_s(D16,G16*-1)","v":11.873694252587784},513.31739319752194]
[5,2467,4568340,77.924586169826185,{"$f":"qo_available(C17,D17)","v":2467.0000000059754},120,-42.075413830173815,{"$f":"(B17*$C$6+$C$3*B17*$C$7)/(24*3600)","v":26.268981481481482},{"$f":"deltah_s(D17,G17*-1)","v":19.345228038662658},846.96572850444284]