{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Separator-Data"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Separator-Data","index":0,"n_rows":9,"n_cols":9,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
["Prof. Milan Stanko (NTNU)",null,null,null,"Red is input"]
["SEPARATOR DATA",null,null,null,"Blue is calculated"]
["Internal diameter","[m]",3.5]
["Effective length","[m]",6]
["Normal liquid level","[m]",{"$f":"C3/2","v":1.75}]
["Distance between shutdown level and normal liquid level","[m]",0.8]
["Liquid cross section area (at normal liquid level)","[m2]",null,null,null,null,null,null,"This equation is available as a UDF, name “Aw”"]
["Liquid cross section area (at shutdown liquid level)","[m2]"]
["Liquid volume between normal liquid level and shutdown","[m3]"]