{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Data"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Data","index":0,"n_rows":15,"n_cols":8,"rows_kept":15,"cut":false,"hidden":false,"merged":[[11,3,11,5],[11,6,11,7]]}
["Problem 6, Exam TPG4230 (resit), V2024, Prof. Milan Stanko"]
[]
["Deterministic variables"]
["field plateau rate, qpf","[Sm3/d]",20000000]
["well production potential at initial time, qppow","[Sm3/d]",5700000]
["Number of producer wells, Nw","[-]",9]
["uptime, tuptime","[d/y]",360]
["discount rate, i","[-]",0.05]
["gas price, Pg","[USD/Sm3]",0.1]
["Abandonment time, tend","[y]",31]
[]
[null,null,null,"Triangular dist.",null,null,"Normal dist"]
["Probabilistic variables",null,"Distribution","min","max","mode","mean","stddev"]
["Initial gas in place, G","[Sm3]","Normal",null,null,null,270000000000,20000000000]
["time to production startup, tini","[y]","Triangular",3,7,5]