{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Data"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":7,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Data","index":0,"n_rows":11,"n_cols":8,"rows_kept":11,"cut":false,"hidden":false,"merged":[[7,3,7,5]]}
["Exercise set 2, Problem 2, Prof. Milan Stanko (NTNU)",null,null,null,"TPR:"]
[]
[null,"pR","[bara]",300,null,"Coefficients for TPR"]
[null,null,null,null,null,"a","[bara/(Sm3/d)^2]",5.0899999999999997E-5]
[null,null,null,null,null,"b","[bara/Sm3/d]",4.1999999999999997E-3]
[null,null,null,null,null,"c","[bara]",198]
[]
[null,null,null,"IPR",null,null,"TPR"]
[null,null,null,"pwf","J","qo","pwf","error"]
[null,null,null,"[bara]","[Sm3/d/bar]","[Sm3/d]","[bara]","[bara]"]
[null,null,null,null,1.75]