{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["Input","Composition","PVT","T_vs_x"],"not_rendered":{"charts":2,"images":0,"macros":1,"external_links":0,"defined_names":27,"comments":0,"pivot_tables":0},"unopened":[{"sheet":"T_vs_x","index":3,"reason":"not_a_worksheet"}],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Input","index":0,"n_rows":24,"n_cols":8,"rows_kept":24,"cut":false,"hidden":false,"merged":[]}
["Problem 2, Prof Milan Stanko (NTNU)"]
["qo","[Sm3/d]"]
["qg","[Sm3/d]"]
["deno_sc","[kg/m3]"]
["deng_sc","[kg/m3]"]
["mass flow","[kg/s]"]
["U","[W/m2 K]",10]
["ID","[m]",7.2999999999999995E-2]
[null,null,null,null,"Formation Temp",null,"SUM="]
["MD","p","T","enthalpy","Tformation","Q","enthalpy_calc","error"]
["[m]","[bara]","[C]","[kJ/kg]","[C]","[W]","[kJ/kg]","[kJ/kg]^2"]
[0,null,null,null,15]
[250,null,null,null,{"$f":"lininterpol($A$12,$E$12,$A$24,$E$24,A13)","v":21.25}]
[500,null,null,null,27.5]
[750,null,null,null,33.75]
[1000,null,null,null,40]
[1250,null,null,null,46.25]
[1500,null,null,null,52.5]
[1750,null,null,null,58.75]
[2000,null,null,null,65]
[2250,null,null,null,71.25]
[2500,null,null,null,77.5]
[2750,null,null,null,{"$f":"lininterpol($A$12,$E$12,$A$24,$E$24,A23)","v":83.75}]
[3000,null,90,null,90]

{"sheet":"Composition","index":1,"n_rows":16,"n_cols":2,"rows_kept":16,"cut":false,"hidden":false,"merged":[]}
["GOR",290.39999999999998]
[null,"Mole fraction"]
["z-N2",4.9678030022644497E-3]
["z-CO2",1.4629880934377E-3]
["z-C1",0.57979574759180097]
["z-C2",6.1219337600781597E-2]
["z-C3",3.2853066289271898E-2]
["z-i-C4",1.3931491299188199E-2]
["z-n-C4",8.0898983528162292E-3]
["z-i-C5",6.1658979371588098E-3]
["z-n-C5",3.6037164761367098E-3]
["z-n-C6",1.2245151644965801E-2]
["z-n-C7",2.6708019028922E-2]
["z-n-C8",3.18321686052132E-2]
["z-n-C9",2.44052606243754E-2]
["z-n-C10",0.19271945256572701]

{"sheet":"PVT","index":2,"n_rows":27,"n_cols":3,"rows_kept":27,"cut":false,"hidden":false,"merged":[]}
["p","T","h"]
["[bara]","[C]","[kJ/kg]"]
[80,20,{"$f":"2.0934*B3","v":41.867999999999995}]
[80,40,83.73599999999999]
[80,60,125.604]
[80,80,167.47199999999998]
[80,100,209.34]
[100,20,41.867999999999995]
[100,40,83.73599999999999]
[100,60,125.604]
[100,80,167.47199999999998]
[100,100,209.34]
[120,20,41.867999999999995]
[120,40,83.73599999999999]
[120,60,125.604]
[120,80,167.47199999999998]
[120,100,209.34]
[140,20,41.867999999999995]
[140,40,83.73599999999999]
[140,60,125.604]
[140,80,167.47199999999998]
[140,100,209.34]
[160,20,41.867999999999995]
[160,40,83.73599999999999]
[160,60,125.604]
[160,80,167.47199999999998]
[160,100,209.34]