{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Data"],"not_rendered":{"charts":2,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Data","index":0,"n_rows":46,"n_cols":10,"rows_kept":46,"cut":false,"hidden":false,"merged":[[18,7,18,9]]}
["Problem 1, Resit Exam TPG4245, Prof. Milan Stanko"]
[]
["Tubing tables (pwf values with pwh=30 bara, and different GORs in the tubing)"]
["qo","GOR","pwf"]
["[Sm3/d]","[Sm3/Sm3]","[bara]",null,"IPR"]
[0.1,54,185.27351271623616,null,"pR","[bara]",200]
[1,54,185.13075503408174,null,"qomax","[Sm3/d]",3000]
[10,54,183.87601571574854,null,"GORR","[Sm3/Sm3]",54]
[50,54,180.72597588429727]
[100,54,179.22943362749299,null,"pwf","qo"]
[250,54,181.21029044902451,null,"[bara]","[Sm3/d]"]
[500,54,190.79618296270732]
[750,54,200.90282428205623]
[1000,54,211.42445227997405]
[2000,54,255.59753416599403]
[0.1,100,180.36507118633179]
[1,100,179.74312907755075]
[10,100,174.29734152360771,null,"Gas lift performance curve"]
[50,100,159.72840342169624,null,null,null,null,"For solving using goal Seek only"]
[100,100,151.28884804260406,null,"GOR","qo(IPR)","qginj","pwf(IPR)","pwf(TPR)","pwf(IPR)-pwf(TPR)"]
[250,100,146.66870793862458,null,"[Sm3/Sm3]","[Sm3/d]","[Sm3/d]","[bara]","[bara]","[bar]"]
[500,100,154.31861543819431,null,54]
[750,100,166.05704599898775,null,100]
[1000,100,178.62874463978986,null,300]
[2000,100,225.64930548732522,null,700]
[0.1,300,174.68985257133386]
[1,300,171.91583394504136]
[10,300,149.31941428488116]
[50,300,108.50094856738775]
[100,300,96.559455166162337]
[250,300,94.831790522759093]
[500,300,105.96234213761706]
[750,300,119.02601449033973]
[1000,300,141.48138301723014]
[2000,300,237.38791510195958]
[0.1,500,173.21172927927938]
[0.1,700,172.50815596163491]
[1,700,165.27865774929481]
[10,700,118.40495983077636]
[50,700,76.088402006240912]
[100,700,71.444565779687451]
[250,700,77.719469625844695]
[500,700,108.75389099538084]
[750,700,138.18993872220514]
[1000,700,174.43612053046019]
[2000,700,364.90040221449573]